{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":39,"n_cols":7,"rows_kept":39,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","5XXM-A"]
[]
[]
[]
[]
["","","","","","5XXM68A2V1B","5XXM90A2V1B"]
["Dimensions","Unit","","Height","mm","734","734"]
["","","","Width","mm","1040","1040"]
["","","","Depth","mm","408","408"]
["Weight","Unit","","","kg","69.0","73.0"]
["Compressor","Type","","","","Hermetically sealed swing compressor","Hermetically sealed swing compressor"]
["Operation range","Cooling","Ambient","Min.","°CDB","-10","-10"]
["","","","Max.","°CDB","50","50"]
["Sound pressure level","Cooling","","Nom.","dBA","48.0 (2)","52.0 (2)"]
["","Heating","","Nom.","dBA","49.0 (2), 51.0 (3)","53.0 (2), 55.0 (3)"]
["Refrigerant","Type","","","","R-32","R-32"]
["","Charge","","","kg","2.00","2.40"]
["","Charge","","","tCO2Eq","1.35","1.62"]
["","GWP","","","","675","675.0"]
["Piping connections","Piping length","OU - IU","Max.","m","25 (4) (5)","25 (5) (4)"]
["","Additional refrigerant charge","","","kg/m","0.02 (for piping length exceeding 30m) (2)","0.02 (for piping length exceeding 30m)"]
["","Level difference","IU - OU","Max.","m","15.0 (5)","15.0 (5)"]
["","","IU - IU","Max.","m","7.5 (5)","7.5 (5)"]
["","Total piping length","System","Actual","m","60","75"]
["Standard Accessories","Installation manual","","","","1","1"]
["","Drain cap","","","","3","3"]
["","Drain plug","","","","1","1"]
["","Reducer assembly","","","","1","1"]
["","Screw bag","","","","2","2"]
["Energy Efficiency Range","","","","","A+++ ~ D","A+++ ~ D"]
["Power supply","Phase","","","","1~","1~"]
["","Frequency","","","Hz","50","50"]
["","Voltage","","","V","220-240","220-240"]
["Notes","","","","","(1) - See separate drawings for operation range","(1) - See separate drawings for operation range"]
["","","","","","(2) - For DX combination","(2) - For DX combination"]
["","","","","","(3) - For Space heating operation of CHVX07 unit","(3) - For Space heating operation of CHVX07 unit"]
["","","","","","(4) - For one room","(4) - For one room"]
["","","","","","(5) - For combination with FBA71/100/125 refer to installation manual","(5) - For combination with FBA71/100/125 refer to installation manual"]
["","","","","","(6) - Contains fluorinated greenhouse gases","(6) - Contains fluorinated greenhouse gases"]