{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":6,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ABQ-C / AZQS-BY1"]
[]
[]
[]
[]
["","","","","ABQ100CV1 / AZQS100B7Y1B","ABQ125CV1 / AZQS125B7Y1B"]
["Cooling capacity","Nom.","","kW","9.5","12.1 (1)"]
["Space cooling","SEER","","","4.65","4.68"]
["","Annual energy consumption","","kWh/a","716","1,550"]
["","Capacity","Pdesign","kW","9.50","12.1"]
["","Energy efficiency class","","","B"]
["Space heating (Average climate)","Capacity","Pdesign","kW","6.78","8.13"]
["","SCOP/A","","","3.80","3.41"]
["","Energy efficiency class","","","A"]
["","Annual energy consumption","","kWh/a","2,498","3,340"]
["Nominal efficiency","EER","","","2.62","2.27 (3)"]
["","Annual energy consumption","","kWh","1,813"]
["","COP","","","3.42"]
["","Energy labeling Directive","Cooling","","D"]
["","","Heating","","B"]
["Heating capacity","Nom.","","kW","10.8","13.5 (2)"]
["Notes","","","","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 7.5m; level difference: 0m"]
["","","","","(2) - Annual energy consumption is according to Energy labeling directive 2002/31/EC","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 7.5m; level difference: 0m"]
["","","","","(3) - SEER and SCOP are according to EN 14825","(3) - EER/COP according to Eurovent 2012, for use outside EU only"]
["","","","","(4) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load"]