{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":45,"n_cols":9,"rows_kept":45,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ADEA-A / ARXM-N9"]
[]
[]
[]
[]
["","","","","ADEA35A2VEB / ARXM35N2V1B9","ADEA35A2VEB / ARXM35N5V1B9","ADEA50A2VEB / ARXM50N2V1B9","ADEA60A2VEB / ARXM60N2V1B9","ADEA71A2VEB / ARXM71N2V1B9"]
["Cooling capacity","Nom.","","kW","3.40","3.40","5.00","5.70"]
["Space cooling","SEER","","","5.75","5.75","5.65","5.74"]
["","Annual energy consumption","","kWh/a","207","207","310","347"]
["","Capacity","Pdesign","kW","3.40","3.40","5.00","5.70"]
["","Energy efficiency class","","","A+","A+","A+","A+"]
["Space heating (Average climate)","Capacity","Pdesign","kW","2.90","2.90","4.40","4.60"]
["","SCOP/A","","","4.00","4.00","4.00","4.00"]
["","Energy efficiency class","","","A+","A+","A+","A+"]
["","Pdh Heating capacity at -10°","","kW","2.41","2.41","3.73","4.00"]
["","Annual energy consumption","","kWh/a","1,014","1,014","1,538","1,610"]
["Nominal efficiency","Annual energy consumption","","kWh","452","452","765","831"]
["","EER","","","3.76","3.76","3.27","3.43"]
["","COP","","","3.97","3.97","3.74","3.63"]
["","Energy labeling Directive","Cooling","","A","A","A","A"]
["","","Heating","","A","A","A","A"]
["Heating capacity","Nom.","","kW","4.00","4.00","5.50","7.00"]
["Notes","","","","(1) - See separate drawing for operation range","(1) - See separate drawing for operation range","(1) - See separate drawing for operation range","(1) - See separate drawing for operation range"]
["","","","","(2) - See separate drawing for electrical data","(2) - See separate drawing for electrical data","(2) - See separate drawing for electrical data","(2) - See separate drawing for electrical data"]
["","","","","(3) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(3) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(3) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(3) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(4) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(4) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(4) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(4) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["Cooling capacity","Nom.","","kW","","","","","6.80"]
["","Max.","","kW","","","","","6.98"]
["Heating capacity","Nom.","","kW","","","","","7.50"]
["","Max.","","kW","","","","","7.66"]
["Nominal efficiency","EER","","","","","","","2.95"]
["","COP","","","","","","","3.49"]
["","Annual energy consumption","","kWh","","","","","1153"]
["","Energy labeling Directive","Cooling","","","","","","C"]
["","","Heating","","","","","","B"]
["Space cooling","Energy efficiency class","","","","","","","A"]
["","Capacity","Pdesign","kW","","","","","6.80"]
["","SEER","","","","","","","5.35"]
["","Annual energy consumption","","kWh/a","","","","","445"]
["Space heating (Average climate)","Energy efficiency class","","","","","","","A"]
["","Capacity","Pdesign","kW","","","","","6.00"]
["","SCOP/A","","","","","","","3.80"]
["","Pdh Heating capacity at -10°","","kW","","","","","4.83"]
["","Annual energy consumption","","kWh/a","","","","","2209"]
["Energy Efficiency Range","","","","","","","","A+++ ~ D"]