{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":10,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATX-K / ARX-K"]
[]
[]
[]
[]
["","","","","ATX20KV1B / ARX20K2V1B","ATX20KV1B / ARX20K5V1B9","ATX25KV1B / ARX25K2V1B","ATX25KV1B / ARX25K5V1B9","ATX35KV1B / ARX35K2V1B","ATX35KV1B / ARX35K5V1B9"]
["Cooling capacity","Min.","","kW","1.3","1.3","1.3","1.3","1.3","1.3"]
["","Max.","","kW","2.6","2.6","3.0","3.0","4.0","4.0"]
["","Nom.","","kW","2.0 (2)","2.0 (2)","2.5 (2)","2.5 (2)","3.5 (2)","3.5 (2)"]
["Space cooling","SEER","","","6.62","6.62","6.46","6.46","6.40","6.40"]
["","Annual energy consumption","","kWh/a","106","106","135","135","181","181"]
["","Capacity","Pdesign","kW","2.00","2.00","2.50","2.50","3.50","3.50"]
["","Energy efficiency class","","","A++","A++","A++","A++","A++","A++"]
["Space heating (Average climate)","Capacity","Pdesign","kW","2.20","2.20","2.40","2.40","2.80","2.80"]
["","SCOP/A","","","4.64","4.64","4.60","4.60","4.62","4.62"]
["","Energy efficiency class","","","A++","A++","A++","A++","A++","A++"]
["","Annual energy consumption","","kWh/a","664","664","730","730","849","849"]
["Piping connections","Liquid","OD","mm","6.35","6.35","6.35","6.35","6.35","6.35"]
["","Gas","OD","mm","9.5","9.5","9.5","9.5","9.5","9.5"]
["","Drain","OD","mm","18","18","18","18","18","18"]
["Nominal efficiency","EER","","","3.97 (1)","3.97 (1)","3.78 (1)","3.78 (1)","3.43 (1)","3.43 (1)"]
["","Annual energy consumption","","kWh","252","252","331","331","510","510"]
["","COP","","","4.77 (1)","4.77 (1)","4.36 (1)","4.36 (1)","4.02 (1)","4.02 (1)"]
["","Energy labeling Directive","Cooling","","A","A","A","A","A","A"]
["","","Heating","","A","A","A","A","A","A"]
["Heating capacity","Nom.","","kW","2.5 (2)","2.5 (2)","3.0 (2)","3.0 (2)","4.0 (2)","4.0 (2)"]
["","Min.","","kW","1.3","1.3","1.3","1.3","1.3","1.3"]
["","Max.","","kW","3.5","3.5","4.0","4.0","4.8","4.8"]
["Notes","","","","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only"]
["","","","","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load"]