{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":9,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXF-A / 2AMXF-A"]
[]
[]
[]
[]
["","","","","ATXF25A5V1B / ATXF25A5V1B / 2AMXF40A2V1B","ATXF25A5V1B / ATXF35A5V1B / 2AMXF40A2V1B","ATXF25A5V1B / ATXF25A5V1B / 2AMXF50A2V1B","ATXF25A5V1B / ATXF35A5V1B / 2AMXF50A2V1B","ATXF35A5V1B / ATXF35A5V1B / 2AMXF50A2V1B"]
["Cooling capacity","Nom.","","kW","4","4","5","5","5"]
["Heating capacity","Nom.","","kW","4.2","4.2","5.6","5.6","5.6"]
["Nominal efficiency","EER","","","3.48","3.53","3.35","3.37","3.38"]
["","COP","","","4.06","4.14","3.71","3.73","3.75"]
["","Annual energy consumption","","kWh","575","570","747","742","740"]
["","Energy labeling Directive","Cooling","","A","A","A","A","A"]
["","","Heating","","A","A","A","A","A"]
["Space cooling","Energy efficiency class","","","A++","A++","A++","A++","A++"]
["","Capacity","Pdesign","kW","4","4","5","5","5"]
["","SEER","","","7","6.93","7.1","7.1","7"]
["","Annual energy consumption","","kWh/a","200","202","247","246","250"]
["Space heating (Average climate)","Energy efficiency class","","","A+","A+","A+","A+","A+"]
["","Capacity","Pdesign","kW","3.2","3.2","4.2","4.2","4.2"]
["","SCOP/A","","","4.01","4","4.1","4.1","4.1"]
["","Pdh Heating capacity at -10°","","kW","2.46","2.46","3.32","3.32","3.32"]
["","Annual energy consumption","","kWh/a","1116","1119","1434","1434","1434"]
["Energy Efficiency Range","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Notes","","","","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]