{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":5,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXF-A / ARXF-F"]
[]
[]
[]
[]
["","","","","ATXF50A2V1B / ARXF50F5V1B"]
["Outdoor unit","","","","ARXF50F5V1B"]
["Cooling capacity","Min.","","kW","1.3"]
["","Nom.","","kW","5"]
["","Max.","","kW","5.3"]
["Heating capacity","Min.","","kW","1.43"]
["","Nom.","","kW","5.4"]
["","Max.","","kW","6.13"]
["Nominal efficiency","EER","","","3.27"]
["","COP","","","3.71"]
["","Annual energy consumption","","kWh","271"]
["","Energy labeling Directive","Cooling","","A"]
["","","Heating","","A"]
["Space cooling","Energy efficiency class","","","A++"]
["","Capacity","Pdesign","kW","5"]
["","SEER","","","6.45"]
["","Annual energy consumption","","kWh/a","271"]
["Space heating (Average climate)","Energy efficiency class","","","A+"]
["","Capacity","Pdesign","kW","3.8"]
["","SCOP/A","","","4.07"]
["","Pdh Heating capacity at -10°","","kW","3.24"]
["","Annual energy consumption","","kWh/a","1309"]
["Notes","","","","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m. Data for high efficiency series, Eurovent certified"]
["","","","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m. Data for standard efficiency series"]
["","","","","(3) - See separate drawing for electrical data"]