{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":47,"n_cols":7,"rows_kept":47,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXF-A"]
[]
[]
[]
[]
["","","","","","ATXF50A2V1B","ATXF60A2V1B"]
["Sound pressure level","Heating","","High","dBA","42","44"]
["","","","Medium","dBA","38","40"]
["","","","Silent operation","dBA","30","32"]
["","","","Low","dBA","33","35"]
["","Cooling","","Medium","dBA","39","41"]
["","","","Silent operation","dBA","31","33"]
["","","","Low","dBA","34","36"]
["","","","High","dBA","43","45"]
["Standard Accessories","AAA dry-cell batteries","","","","2","2"]
["","Installation manual","","","","1","1"]
["","Operation manual","","","","1","1"]
["","Infrared remote control","","","","1","1"]
["","Remote control holder","","","","1","1"]
["","Mounting plate","","","","1","1"]
["","Indoor unit fixing screws","","","","2","2"]
["Control systems","Wired remote control","","","","BRC073A1","BRC073A1"]
["","Infrared remote control","","","","ARC470A1","ARC470A1"]
["Piping connections","Liquid","","OD","mm","6.35","6.35"]
["","Gas","","OD","mm","12.7","12.7"]
["","Drain","","","","18","18"]
["Power input","Cooling","","Nom.","kW","0.029","0.032"]
["","Heating","","Nom.","kW","0.032","0.035"]
["Sound power level","Cooling","","","dBA","59","60"]
["","Heating","","","dBA","61","62"]
["Dimensions","Unit","","Width","mm","990","990"]
["","","","Depth","mm","263","263"]
["","","","Height","mm","295","295"]
["Casing","Colour","","","","White","White"]
["Weight","Unit","","","kg","13.5","13.5"]
["Fan","Air flow rate","Heating","High","m³/min","17.3","17.9"]
["","","","Medium","m³/min","14.8","15.8"]
["","","","Low","m³/min","12.2","12.8"]
["","","","Silent operation","m³/min","10.7","11.3"]
["","","Cooling","Low","m³/min","11.9","12.2"]
["","","","Medium","m³/min","14.4","14.8"]
["","","","High","m³/min","16.8","17.3"]
["","","","Silent operation","m³/min","10.5","10.7"]
["Power supply","Phase","","","","1~","1~"]
["","Name","","","","V1","V1"]
["","Frequency","","","Hz","50","50"]
["","Voltage","","","V","220-240","220-240"]