{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":28,"n_cols":8,"rows_kept":28,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXF-C / ARXF-D"]
[]
[]
[]
[]
["","","","","ATXF20C5V1B / ARXF20D5V1B","ATXF25C5V1B / ARXF25D5V1B","ATXF35C5V1B / ARXF35D5V1B","ATXF42C5V1B / ARXF42D5V1B"]
["Cooling capacity","Min.","","kW","1.3","1.3","1.3","1.4"]
["","Max.","","kW","2.4","2.8","3.8","4.3"]
["","Nom.","","kW","2.00","2.50","3.30","4.20"]
["Space cooling","SEER","","","6.40","6.40","6.40","6.45"]
["","Annual energy consumption","","kWh/a","109","137","191","228"]
["","Capacity","Pdesign","kW","2.00","2.50","3.50","4.20"]
["","Energy efficiency class","","","A++","A++","A++","A++"]
["Space heating (Average climate)","Capacity","Pdesign","kW","2.20","2.40","2.60","3.30"]
["","SCOP/A","","","4.07","4.01","4.01","4.25"]
["","Energy efficiency class","","","A+","A+","A+","A+"]
["","Pdh Heating capacity at -10°","","kW","1.91","2.00","2.22","2.61"]
["","Annual energy consumption","","kWh/a","757","837","907","1,086"]
["Nominal efficiency","EER","","","3.33","3.24","3.27","3.27"]
["","COP","","","3.75","3.73","3.72","3.71"]
["","Energy labeling Directive","Cooling","","A","A","A","A"]
["","","Heating","","A","A","A","A"]
["Heating capacity","Nom.","","kW","2.40","2.80","3.50","4.60"]
["","Min.","","kW","1.30","1.30","1.30","1.40"]
["","Max.","","kW","3.30","3.70","4.40","5.00"]
["Notes","","","","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m. Data for high efficiency series, Eurovent certified","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m. Data for high efficiency series, Eurovent certified","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m. Data for high efficiency series, Eurovent certified","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m. Data for high efficiency series, Eurovent certified"]
["","","","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m. Data for standard efficiency series","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m. Data for standard efficiency series","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m. Data for standard efficiency series","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m. Data for standard efficiency series"]
["","","","","(3) - See separate drawing for electrical data","(3) - See separate drawing for electrical data","(3) - See separate drawing for electrical data","(3) - See separate drawing for electrical data"]