{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":7,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXF-F / 2AMXF-B"]
[]
[]
[]
[]
["","","","","ATXF25F5V1B / ATXF25F5V1B  / 2AMXF40B2V1B","ATXF25F5V1B / ATXF25F5V1B / 2AMXF40B2V1B","ATXF25F5V1B / ATXF25F5V1B / 2AMXF50B2V1B"]
["Cooling capacity","Nom.","","kW","4.00","4.00","5.0"]
["Heating capacity","Nom.","","kW","4.20","4.20","5.60"]
["Nominal efficiency","EER","","","3.48","3.48","3.35"]
["","COP","","","4.06","4.06","3.71"]
["","Annual energy consumption","","kWh","575","575","747"]
["","Energy labeling Directive","Cooling","","A","A","A"]
["","","Heating","","A","A","A"]
["Space cooling","Energy efficiency class","","","A++","A++","A++"]
["","Capacity","Pdesign","kW","4.00","4.00","5.00"]
["","SEER","","","7.00","7.00","7.10"]
["","Annual energy consumption","","kWh/a","200","200","247"]
["Space heating (Average climate)","Energy efficiency class","","","A++","A++","A++"]
["","Capacity","Pdesign","kW","3.20","3.20","4.20"]
["","SCOP/A","","","4.60","4.60","4.60"]
["","Pdh Heating capacity at -10°","","kW","2.79","2.79","3.32"]
["","Annual energy consumption","","kWh/a","973","973","1277"]
["Notes","","","","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]