{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":8,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXM-R / ARXM-R9"]
[]
[]
[]
[]
["","","","","ATXM25R2V1B / ARXM25R5V1B9","ATXM25R5V1B / ARXM25R5V1B9","ATXM35R2V1B / ARXM35R5V1B9","ATXM35R5V1B / ARXM35R5V1B9"]
["Cooling capacity","Min.","","kW","1.30","1.30","1.40","1.40"]
["","Max.","","kW","3.20","3.20","4.00","4.00"]
["","Nom.","","kW","2.50","2.50","3.40","3.40"]
["Space cooling","SEER","","","8.55","8.55","8.55","8.55"]
["","Annual energy consumption","","kWh/a","102","102","139","139"]
["","Capacity","Pdesign","kW","2.50","2.50","3.40","3.40"]
["","Energy efficiency class","","","A+++","A+++","A+++","A+++"]
["Space heating (Average climate)","Capacity","Pdesign","kW","2.40","2.40","2.50","2.50"]
["","SCOP/A","","","5.10","5.10","5.10","5.10"]
["","Energy efficiency class","","","A+++","A+++","A+++","A+++"]
["","Pdh Heating capacity at -10°","","kW","","","2.35"]
["","Annual energy consumption","","kWh/a","659","659","686","686"]
["Nominal efficiency","Annual energy consumption","","kWh","278","278","402","402"]
["","EER","","","4.50","4.50","4.23","4.23"]
["","COP","","","5.00","5.00","4.04","4.04"]
["","Energy labeling Directive","Cooling","","A","A","A","A"]
["","","Heating","","A","A","A","A"]
["Heating capacity","Nom.","","kW","2.80","2.80","4.00","4.00"]
["","Min.","","kW","1.30","1.30","1.40","1.40"]
["","Max.","","kW","4.70","4.70","5.20","5.20"]
["Notes","","","","(1) - See separate drawing for operation range","(1) - See separate drawing for operation range","(1) - See separate drawing for operation range","(1) - See separate drawing for operation range"]
["","","","","(2) - See separate drawing for electrical data","(2) - See separate drawing for electrical data","(2) - See separate drawing for electrical data","(2) - See separate drawing for electrical data"]
["","","","","(3) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(3) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(3) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(3) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(4) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(4) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(4) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(4) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]