{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":46,"n_cols":6,"rows_kept":46,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","AVA-A"]
[]
[]
[]
[]
["","","","","","AVA125AMVE"]
["Cooling capacity","Total capacity","","Nom.","kW","12.10"]
["Heating capacity","Total capacity","","Nom.","kW","13.5"]
["Casing","Colour","","","","Fresh White"]
["Dimensions","Unit","","Height","mm","1850"]
["","","","Width","mm","600"]
["","","","Depth","mm","350"]
["Weight","Unit","","","kg","50"]
["Fan","Air flow rate","Cooling","High","m³/min","28"]
["","","","Medium","m³/min","26"]
["","","","Low","m³/min","24"]
["","","Heating","High","m³/min","28"]
["","","","Medium","m³/min","26"]
["","","","Low","m³/min","24"]
["Sound power level","Cooling","","","dBA","63"]
["Sound pressure level","Cooling","","High","dBA","51"]
["","","","Medium","dBA","48"]
["","","","Low","dBA","46"]
["","Heating","","High","dBA","51"]
["","","","Medium","dBA","46"]
["","","","Nom.","dBA","48"]
["Piping connections","Liquid","","OD","mm","9.52"]
["","Gas","","OD","mm","15.9"]
["","Drain","","","","I.D. 20/O.D. 26"]
["Control systems","Wired remote control","","","","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7"]
["Standard Accessories","Installation manual","","","","1"]
["","Hole protection rubber","","","","2"]
["","Cover","","","","1"]
["","Dew proof material","","","","1"]
["","Remote control wiring","","","","1"]
["","Bracket for installation","","","","1"]
["","Operation manual","","","","1"]
["","Bush","","","","1"]
["","Installation pattern","","","","1"]
["","Insulation for fitting for gas pipe","","","","1"]
["","Insulation for fitting for liquid pipe","","","","1"]
["","Screws","","","","5"]
["","Tie-wraps","","","","5"]
["Power supply","Phase","","","","1~"]
["","Frequency","","","Hz","50/60"]
["","Voltage","","","V","220-240/220"]