{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":6,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXM-R / 5MXM-N9"]
[]
[]
[]
[]
["","","","","CTXM15R2V1B / FTXM71R2V1B / 5MXM90N2V1B9","CTXM15R5V1B / FTXM71R2V1B / 5MXM90N2V1B9"]
["Cooling capacity","Nom.","","kW","8.00","8.00"]
["Space cooling","SEER","","","6.84","6.84"]
["","Annual energy consumption","","kWh/a","410","410"]
["","Capacity","Pdesign","kW","8.00","8.00"]
["","Energy efficiency class","","","A+++","A+++"]
["Space heating (Average climate)","Capacity","Pdesign","kW","4.50","4.50"]
["","SCOP/A","","","4.28","4.28"]
["","Energy efficiency class","","","A+","A+"]
["","Annual energy consumption","","kWh/a","1,472","1,472"]
["Nominal efficiency","EER","","","3.33","3.33"]
["","Annual energy consumption","","kWh","1,202","1,202"]
["","COP","","","3.67","3.67"]
["","Energy labeling Directive","Cooling","","A","A"]
["","","Heating","","A","A"]
["Heating capacity","Nom.","","kW","10.00","10.00"]
["Notes","","","","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range"]
["","","","","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data"]