{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":29,"n_cols":12,"rows_kept":29,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CYQL-DK-F"]
[]
[]
[]
[]
["","","","","CYQL100DK125FBN","CYQL100DK125FSN","CYQL150DK200FBN","CYQL150DK200FSN","CYQL200DK250FBN","CYQL200DK250FSN","CYQL250DK250FBN","CYQL250DK250FSN"]
["Door width","Max.","","m","1.0","1.0","1.5","1.5","2.0","2.0","2.5","2.5"]
["Refrigerant","GWP","","","2,087.5","2,087.5","2,087.5","2,087.5","2,087.5","2,087.5","2,087.5","2,087.5"]
["","Type","","","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A"]
["Dimensions","Unit","Width","mm","1,000","1,000","1,500","1,500","2,000","2,000","2,500","2,500"]
["","","Depth","mm","774","774","774","774","774","774","774","774"]
["","","Height","mm","370","370","370","370","370","370","370","370"]
["Casing","Material","","","Electro-galvanised sheet steel","Electro-galvanised sheet steel","Electro-galvanised sheet steel","Electro-galvanised sheet steel","Electro-galvanised sheet steel","Electro-galvanised sheet steel","Electro-galvanised sheet steel","Electro-galvanised sheet steel"]
["","Colour","","","RAL9016","RAL9006","RAL9016","RAL9006","RAL9016","RAL9006","RAL9016","RAL9006"]
["Weight","Unit","","kg","76","76","100","100","126","126","157","157"]
["Door height","Max.","","m","3.0 (2), 2.75 (3), 2.5 (4)","3.0 (2), 2.75 (3), 2.5 (4)","3.0 (2), 2.75 (3), 2.5 (4)","3.0 (2), 2.75 (3), 2.5 (4)","3.0 (2), 2.75 (3), 2.5 (4)","3.0 (2), 2.75 (3), 2.5 (4)","3.0 (2), 2.75 (3), 2.5 (4)","3.0 (2), 2.75 (3), 2.5 (4)"]
["Piping connections","Liquid","OD","mm","9.52","9.52","9.52","9.52","9.52","9.52","9.52","9.52"]
["","Gas","OD","mm","16.0","16.0","19.0","19.0","22.0","22.0","22.0","22.0"]
["Power input","Fan only","Nom.","kW","0.75","0.75","1.13","1.13","1.50","1.50","1.88","1.88"]
["Required ceiling void >","mm","","","520","520","520","520","520","520","520","520"]
["Power supply","Frequency","","Hz","50","50","50","50","50","50","50","50"]
["","Voltage","","V","230","230","230","230","230","230","230","230"]
["Notes","","","","(1) - Installation level B: standard setting, refer to the databook of installation manual for more information (only one installation level available)","(1) - Installation level B: standard setting, refer to the databook of installation manual for more information (only one installation level available)","(1) - Installation level B: standard setting, refer to the databook of installation manual for more information (only one installation level available)","(1) - Installation level B: standard setting, refer to the databook of installation manual for more information (only one installation level available)","(1) - Installation level B: standard setting, refer to the databook of installation manual for more information (only one installation level available)","(1) - Installation level B: standard setting, refer to the databook of installation manual for more information (only one installation level available)","(1) - Installation level B: standard setting, refer to the databook of installation manual for more information (only one installation level available)","(1) - Installation level B: standard setting, refer to the databook of installation manual for more information (only one installation level available)"]
["","","","","(2) - Favorable conditions: covered shopping mall or revolving door entrance","(2) - Favorable conditions: covered shopping mall or revolving door entrance","(2) - Favorable conditions: covered shopping mall or revolving door entrance","(2) - Favorable conditions: covered shopping mall or revolving door entrance","(2) - Favorable conditions: covered shopping mall or revolving door entrance","(2) - Favorable conditions: covered shopping mall or revolving door entrance","(2) - Favorable conditions: covered shopping mall or revolving door entrance","(2) - Favorable conditions: covered shopping mall or revolving door entrance"]
["","","","","(3) - Normal conditions: little direct wind, no opposite open doors, building with ground floor only","(3) - Normal conditions: little direct wind, no opposite open doors, building with ground floor only","(3) - Normal conditions: little direct wind, no opposite open doors, building with ground floor only","(3) - Normal conditions: little direct wind, no opposite open doors, building with ground floor only","(3) - Normal conditions: little direct wind, no opposite open doors, building with ground floor only","(3) - Normal conditions: little direct wind, no opposite open doors, building with ground floor only","(3) - Normal conditions: little direct wind, no opposite open doors, building with ground floor only","(3) - Normal conditions: little direct wind, no opposite open doors, building with ground floor only"]
["","","","","(4) - Unfavorable conditions: location at a corner or square, multiple floors and/or open stairway","(4) - Unfavorable conditions: location at a corner or square, multiple floors and/or open stairway","(4) - Unfavorable conditions: location at a corner or square, multiple floors and/or open stairway","(4) - Unfavorable conditions: location at a corner or square, multiple floors and/or open stairway","(4) - Unfavorable conditions: location at a corner or square, multiple floors and/or open stairway","(4) - Unfavorable conditions: location at a corner or square, multiple floors and/or open stairway","(4) - Unfavorable conditions: location at a corner or square, multiple floors and/or open stairway","(4) - Unfavorable conditions: location at a corner or square, multiple floors and/or open stairway"]
["","","","","(5) - Sound pressure level (at 3m)","(5) - Sound pressure level (at 3m)","(5) - Sound pressure level (at 3m)","(5) - Sound pressure level (at 3m)","(5) - Sound pressure level (at 3m)","(5) - Sound pressure level (at 3m)","(5) - Sound pressure level (at 3m)","(5) - Sound pressure level (at 3m)"]
["","","","","(6) - Pipe work and electrical connections are on top of the unit","(6) - Pipe work and electrical connections are on top of the unit","(6) - Pipe work and electrical connections are on top of the unit","(6) - Pipe work and electrical connections are on top of the unit","(6) - Pipe work and electrical connections are on top of the unit","(6) - Pipe work and electrical connections are on top of the unit","(6) - Pipe work and electrical connections are on top of the unit","(6) - Pipe work and electrical connections are on top of the unit"]
["","","","","(7) - Contains fluorinated greenhouse gases","(7) - Contains fluorinated greenhouse gases","(7) - Contains fluorinated greenhouse gases","(7) - Contains fluorinated greenhouse gases","(7) - Contains fluorinated greenhouse gases","(7) - Contains fluorinated greenhouse gases","(7) - Contains fluorinated greenhouse gases","(7) - Contains fluorinated greenhouse gases"]