{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":7,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EAVX-D6V"]
[]
[]
[]
[]
["","","","","","EAVX16S23DA6V","EAVX16S18DA6V"]
["Casing","Material","","","","Precoated sheet metal","Precoated sheet metal"]
["Dimensions","Unit","","Height","mm","1850","1650"]
["","","","Width","mm","595","595"]
["","","","Depth","mm","625","625"]
["Weight","Unit","","","kg","118","109"]
["Sound power level","Nom.","","","dBA","44.0 (5)","44.0 (5)"]
["Sound pressure level","Nom.","","","dBA","30.0 (6)","30.0 (6)"]
["Operation range","Heating","Water side","Min.","°C","0 (7)","0 (7)"]
["","","","Max.","°C","0 (7)","0 (7)"]
["","Cooling","Ambient","Min.","°CDB","0 (7)","0 (7)"]
["","","Water side","Min.","°C","0 (7)","0 (7)"]
["","","","Max.","°C","0 (7)","0 (7)"]
["Power supply","Name","","","","See note 9","See note 9"]
["Electric heater","Power supply","","Name","","6V3","6V3"]
["","","","Phase","","1~ / 3~","1~ / 3~"]
["","","","Frequency","Hz","50","50"]
["","","","Voltage","V","230","230"]
["","Recommended fuses","","","A","20.000 (10)","20.000 (10)"]
["Notes","","","","","(1) - Operation area is extended to lower flow rates only in case the unit operates with heat pump only. (Not in startup, no BUH operation, no defrost operation).","(1) - Operation area is extended to lower flow rates only in case the unit operates with heat pump only. (Not in startup, no BUH operation, no defrost operation)."]
["","","","","","(2) - Based on a dT of 45 K","(2) - Based on a dT of 45 K"]
["","","","","","(3) - Including piping + back-up heater; excluding expansion vessel","(3) - Including piping + back-up heater; excluding expansion vessel"]
["","","","","","(4) - Excluding the water in the unit. This minimum water volume is sufficient for most applications. During critical processes extra water may be required.","(4) - Excluding the water in the unit. This minimum water volume is sufficient for most applications. During critical processes extra water may be required."]
["","","","","","(5) - Measured with a pressure drop of 10 kPa in the heating system at an operating condition of leaving water 47-55°C in a room with an ambient of 20°C. DB/WB 7°C/6°.","(5) - Measured with a pressure drop of 10 kPa in the heating system at an operating condition of leaving water 47-55°C in a room with an ambient of 20°C. DB/WB 7°C/6°."]
["","","","","","(6) - Value measured in an anechoic room at 1m distance from the unit. It is a relative value, depending on the distance and acoustic environment. The sound pressure level mentioned is measured with a pressure drop of 10 kPa in the heating system at an operatin","(6) - Value measured in an anechoic room at 1m distance from the unit. It is a relative value, depending on the distance and acoustic environment. The sound pressure level mentioned is measured with a pressure drop of 10 kPa in the heating system at an operatin"]
["","","","","","(7) - Refer to operation range of the unit.","(7) - Refer to operation range of the unit."]
["","","","","","(8) - Depends on operation mode, refer to installation manual.","(8) - Depends on operation mode, refer to installation manual."]
["","","","","","(9) - 4 pole 20 A curve 400V tripping class C (refer to wiring diagram)","(9) - 4 pole 20 A curve 400V tripping class C (refer to wiring diagram)"]