{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":6,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHYHBX-AV3 / EVLQ-CV3"]
[]
[]
[]
[]
["","","","","","EHYHBX08AAV3 / EVLQ08CAV3"]
["Domestic hot water heating","General","","Declared load profile","","XL"]
["","Average climate","","Water heating energy efficiency class","","A"]
["COP","","","","","4.45 (3), 3.42 (4)"]
["Space heating","Average climate water outlet 35°C","General","ηs (Seasonal space heating efficiency)","%","168"]
["","","","Seasonal space heating eff. class","","A++"]
["","","","SCOP","","4.28"]
["","Average climate water outlet 55°C","General","Seasonal space heating eff. class","","A++"]
["","","","ηs (Seasonal space heating efficiency)","%","129"]
["","","","SCOP","","3.29"]
["Cooling capacity","Nom.","","","kW","6.86 (4), 5.36 (4)"]
["","Min.","","","kW","2.50 (3), 2.50 (4)"]
["EER","","","","","3.42 (3), 2.29 (4)"]
["Heating capacity","Nom.","","","kW","7.40 (3), 6.89 (4)"]
["","Min.","","","kW","1.80 (3), 1.80 (4)"]
["","Max.","","","kW","10.0 (3), 9.53 (4)"]
["Power input","Heating","","Nom.","kW","1.66 (3), 2.01 (4)"]
["","Cooling","","Nom.","kW","2.01 (3), 2.34 (4)"]
["Notes","","","","","(1) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 45°C (Dt=5°C)"]
["","","","","","(3) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(4) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )"]
["","","","","","(5) - Tamb 35°C - LWE 7°C (DT=5°C), boiler bypassed"]
["","","","","","(6) - Tamb 35°C - LWE 18°C (DT=5°C), boiler bypassed"]
["","","","","","(7) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C), boiler bypassed"]
["","","","","","(8) - DB/WB 7°C/6°C - LWC 45°C (DT=5°C), boiler bypassed"]