{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":12,"n_cols":7,"rows_kept":12,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKHBRD-ACV1 / ERSQ-AV1"]
[]
[]
[]
[]
["","","","","EKHBRD011ACV1 / ERSQ011AAV1","EKHBRD014ACV1 / ERSQ014AAV1","EKHBRD016ACV1 / ERSQ016AAV1"]
["COP","","","","3.08 (1), 2.50 (2), 4.22 (3)","3.00 (1), 2.48 (2), 3.94 (3)","2.88 (1), 2.41 (2), 3.72 (3)"]
["Heating capacity","Nom.","","kW","11 (1), 11 (2), 11 (3)","14 (1), 14 (2), 14 (3)","16 (1), 16 (2), 16 (3)"]
["Power input","Heating","Nom.","kW","3.57 (1), 4.40 (2), 2.61 (3)","4.66 (1), 5.65 (2), 3.55 (3)","5.57 (1), 6.65 (2), 4.31 (3)"]
["Notes","","","","(1) - EW 55°C; LW 65°C; Dt 10°C; ambient conditions: 7°CDB/6°CWB","(1) - EW 55°C; LW 65°C; Dt 10°C; ambient conditions: 7°CDB/6°CWB","(1) - EW 55°C; LW 65°C; Dt 10°C; ambient conditions: 7°CDB/6°CWB"]
["","","","","(2) - EW 70°C; LW 80°C; Dt 10°C; ambient conditions: 7°CDB/6°CWB","(2) - EW 70°C; LW 80°C; Dt 10°C; ambient conditions: 7°CDB/6°CWB","(2) - EW 70°C; LW 80°C; Dt 10°C; ambient conditions: 7°CDB/6°CWB"]
["","","","","(3) - EW 30°C; LW 35°C; Dt 5°C; ambient conditions: 7°CDB/6°CWB","(3) - EW 30°C; LW 35°C; Dt 5°C; ambient conditions: 7°CDB/6°CWB","(3) - EW 30°C; LW 35°C; Dt 5°C; ambient conditions: 7°CDB/6°CWB"]