{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":17,"n_cols":8,"rows_kept":17,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKHWS-BA3V3"]
[]
[]
[]
[]
["","","","","","EKHWS150BA3V3","EKHWS200BA3V3","EKHWS300BA3V3"]
["Booster heater","Capacity","","","kW","3","3","3"]
["Dimensions","Unit","","Width","mm","595","595","595"]
["","","Height","Tank","mm","945","1,195","1,645"]
["","","","Depth","mm","595","595","595"]
["Casing","Material","","","","Epoxy-coated mild steel","Epoxy-coated mild steel","Epoxy-coated mild steel"]
["","Colour","","","","Neutral white","Neutral white","Neutral white"]
["Tank","Energy efficiency class","","","","C","C","C"]
["","Material","","","","Stainless steel (DIN 1.4521)","Stainless steel (DIN 1.4521)","Stainless steel (DIN 1.4521)"]
["","Water volume","","","l","150","200","285"]
["Weight","Unit","","Empty","kg","42","49","62"]
["Notes","","","","","(1) - Heatloss according to EN12897","(1) - Heatloss according to EN12897","(1) - Heatloss according to EN12897"]