{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":6,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ERGA-EVH7"]
[]
[]
[]
[]
["","","","","","ERGA08EAV3H7"]
["Dimensions","Unit","","Height","mm","740"]
["","","","Width","mm","884"]
["","","","Depth","mm","388"]
["Weight","Unit","","","kg","58.5"]
["Operation range","Cooling","","Min.","°CDB","10"]
["","","","Max.","°CDB","43"]
["","Domestic hot water","","Min.","°CDB","-25"]
["","","","Max.","°CDB","35"]
["Sound power level","Heating","","Nom.","dBA","62 (1)"]
["","Cooling","","Nom.","dBA","62 (1)"]
["Sound pressure level","Heating","","Nom.","dBA","49 (1)"]
["","Cooling","","Nom.","dBA","50 (1)"]
["Refrigerant","Type","","","","R-32"]
["","GWP","","","","675.0"]
["","Charge","","","tCO2Eq","1.01"]
["","Charge","","","kg","1.5"]
["Piping connections","Liquid","","OD","mm","6"]
["","Gas","","OD","mm","15.9"]
["","Drain","","OD","mm","18"]
["","Level difference","IU - OU","Max.","m","30.0"]
["","Heat insulation","","","","Both liquid and gas pipes"]
["Power supply","Name","","","","V3"]
["","Phase","","","","1N~"]
["","Frequency","","","Hz","50"]
["","Voltage","","","V","230"]
["Current","Recommended fuses","","","A","25"]
["Notes","","","","","(1) - Cooling Ta 35°C - LWE 18°C (DT = 5°C); Heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]