{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":59,"n_cols":8,"rows_kept":59,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ERSQ-AV1"]
[]
[]
[]
[]
["","","","","","ERSQ011AAV1","ERSQ014AAV1","ERSQ016AAV1"]
["Sound pressure level","Heating","","Nom.","dBA","","53"]
["Standard Accessories","Installation manual","","","","1","1","1"]
["Refrigerant","GWP","","","","","2,087.5"]
["","Charge","","","kg","","4.5"]
["","Type","","","","","R-410A"]
["Operation range","Heating","","Max.","°CWB","","20"]
["","","","Min.","°CWB","","-20"]
["","Domestic hot water","","Min.","°CDB","","-20"]
["","","","Max.","°CDB","","35"]
["Piping connections","Heat insulation","","","","","Both liquid and gas pipes"]
["","Liquid","","OD","mm","","9.52"]
["","Gas","","OD","mm","","15.9"]
["","Drain","","OD","mm","","26x3"]
["","Level difference","IU - OU","Max.","m","","30"]
["Sound power level","Heating","","Nom.","dBA","","69"]
["Dimensions","Unit","","Width","mm","","900"]
["","","","Depth","mm","","320"]
["","","","Height","mm","","1,345"]
["Weight","Unit","","","kg","","120"]
["Power supply","Phase","","","","","1~"]
["","Name","","","","","V1"]
["","Frequency","","","Hz","","50"]
["","Voltage","","","V","","220-440"]
["Current","Recommended fuses","","","A","","25"]
["Notes","","","","","","(1) - See separate drawing for operation range"]
["","","","","","","(2) - Zmax: In accordance with EN/IEC 61000-3-11, it may be necessary to consult the distribution network operator to ensure that the equipment is connected only to a supply with Zsys (system impedance) ≤ Zmax"]
["","","","","","","(3) - EN/IEC 61000-3-11: European/international technical standard setting the limits for voltage changes, voltage fluctuations and flicker in public low-voltage supply systems for equipment with rated ≤ 75A"]
["","","","","","","(4) - Minimum Ssc (=Short-circuit power) value: Equipment complying with EN/IEC 61000-3-12: European/International Technical Standard setting the limits for harmonic currents produced by equipment connected to public low-voltage systems with input current >16A"]
["","","","","","","(5) - Contains fluorinated greenhouse gases"]
["Dimensions","Unit","","Height","mm","1345","","1345"]
["","","","Width","mm","900","","900"]
["","","","Depth","mm","320","","320"]
["Weight","Unit","","","kg","120","","120"]
["Operation range","Heating","","Min.","°CWB","-20","","-20"]
["","","","Max.","°CWB","20","","20"]
["","Domestic hot water","","Min.","°CDB","-20","","-20"]
["","","","Max.","°CDB","35","","35"]
["Sound power level","Heating","","Nom.","dBA","68","","71"]
["Sound pressure level","Heating","","Nom.","dBA","52","","55"]
["Refrigerant","Type","","","","R-410A","","R-410A"]
["","GWP","","","","2087.5","","2087.5"]
["","Charge","","","tCO2Eq","9.4","","9.4"]
["","Charge","","","kg","4.5","","4.5"]
["Piping connections","Liquid","","OD","mm","9.52","","9.52"]
["","Gas","","OD","mm","15.9","","15.9"]
["","Drain","","OD","mm","26x3","","26x3"]
["","Level difference","IU - OU","Max.","m","30","","30"]
["","Heat insulation","","","","Both liquid and gas pipes","","Both liquid and gas pipes"]
["Power supply","Name","","","","V1","","V1"]
["","Phase","","","","1~","","1~"]
["","Frequency","","","Hz","50","","50"]
["","Voltage","","","V","220-440","","220-440"]
["Current","Recommended fuses","","","A","25","","25"]