{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":7,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ETBX16E9W / EPRA014-018DW"]
[]
[]
[]
[]
["","","","","","ETBX16EF9W / EPRA16DAW1","ETBX16EF9W / EPRA18DAW1"]
["COP","","","","","5.00 (2)","5.00"]
["Space heating","Average climate water outlet 35°C","General","ηs (Seasonal space heating efficiency)","%","190"]
["","","","Seasonal space heating eff. class","","A+++"]
["","","","SCOP","","4.81"]
["","Average climate water outlet 55°C","General","Seasonal space heating eff. class","","A++"]
["","","","ηs (Seasonal space heating efficiency)","%","142"]
["","","","SCOP","","3.63"]
["Cooling capacity","Nom.","","","kW","11.5 (3), 7.88 (4)"]
["EER","","","","","4.11 (3), 2.69 (4)","4.09, 2.68"]
["Heating capacity","Nom.","","","kW","9.00 (2)"]
["","Min.","","","kW","3.96 (1)"]
["","Max.","","","kW","10.44 (1)"]
["Power input","Heating","","Max.","kW","2.32 (5)"]
["","","","Min.","kW","0.90 (5)"]
["","","","Nom.","kW","1.80 (2)"]
["","Cooling","","Nom.","kW","2.80 (3), 2.93 (4)"]
["Notes","","","","","(1) - Capacity according to standard EN14511 and valid for heated water range dT = 3~8°C at Ta 7°C","(1) - Capacity according to standard EN14511 and valid for heated water range dT = 3~8°C at Ta 7°C"]
["","","","","","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(3) - Cooling: EW 23°C; LW 18°C; ambient conditions: 35°CDB","(3) - Cooling: EW 23°C; LW 18°C; ambient conditions: 35°CDB"]
["","","","","","(4) - Cooling: EW 12°C; LW 7°C; ambient conditions: 35°CDB","(4) - Cooling: EW 12°C; LW 7°C; ambient conditions: 35°CDB"]
["","","","","","(5) - Power input is total input of indoor and outdoor units, including the circulation pump; according to EN14511","(5) - Power input is total input of indoor and outdoor units, including the circulation pump; according to EN14511"]
["","","","","","(6) - Test at Ta DB/WB 7°C/6°C. According to EN 16147.","(6) - DB/WB 7°C/6°C - LWC 35°C (dT=5°C) with pump at full speed"]
["","","","","","(7) - DB/WB 7°C/6°C - LWC 35°C (dT=5°C) with pump at full speed"]
["Heating capacity","Min.","","","kW","","4.40"]
["","Nom.","","","kW","","9.00"]
["","Max.","","","kW","","11.60"]
["Cooling capacity","Nom.","","","kW","","12.5, 8.86"]
["Power input","Heating","","Min.","kW","","1.00"]
["","","","Nom.","kW","","1.80"]
["","","","Max.","kW","","2.58"]
["","Cooling","","Nom.","kW","","3.05, 3.31"]
["Space heating","Average climate water outlet 55°C","General","SCOP","","","3.63"]
["","","","Seasonal space heating eff. class","","","A++"]
["","Average climate water outlet 35°C","General","SCOP","","","4.81"]
["","","","Seasonal space heating eff. class","","","A+++"]