{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":6,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ETSX-D"]
[]
[]
[]
[]
["","","","","","ETSX16P30DA"]
["Sound pressure level","Nom.","","","dBA","32.8"]
["Operation range","Cooling","Ambient","Min.","°CDB","10"]
["","","Water side","Max.","°C","22"]
["","","","Min.","°C","5"]
["","Heating","Water side","Max.","°C","70"]
["","","","Min.","°C","15"]
["Sound power level","Nom.","","","dBA","45.6"]
["Dimensions","Unit","","Width","mm","590"]
["","","","Depth","mm","615"]
["","","","Height","mm","1,891"]
["Casing","Material","","","","Impact resistant polypropylene"]
["","Colour","","","","Traffic white (RAL9016) / Dark grey (RAL7011)"]
["Weight","Unit","","","kg","73"]
["PED","Category","","","","Art4.3"]
["Power supply","Phase","","","","1~"]
["","Frequency","","","Hz","50"]
["","Voltage","","","V","230"]
["Electric heater","Power supply","","Frequency","Hz","50"]
["","","","Name","","3V / 9W"]
["","","","Phase","","1~ / 3~"]
["Notes","","","","","(1) - Heatloss according to EN12897"]
["","","","","","(2) - TKW = 10°C/TWW = 40°C/TSP = 50°C"]
["","","","","","(3) - TKW = 10°C/TWW = 40°C/TSP = 60°C"]
["","","","","","(4) - TKW = 10°C/TWW = 40°C/TSP = 65°C"]