{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":28,"n_cols":29,"rows_kept":28,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ETSXB16E7 / EPRA14-18DW7"]
[]
[]
[]
[]
["","","","","","ETSXB16P50EG7 / EPRA14DAW17","ETSXB16P30EG7 / EPRA14DAW17","ETSXB16P30EG7 / EPRA14DBW17","ETSXB16P50EG7 / EPRA14DBW17","ETSXB16P30EF7 / EPRA14DAW17","ETSXB16P50EF7 / EPRA14DAW17","ETSXB16P30EF7 / EPRA14DBW17","ETSXB16P50EF7 / EPRA14DBW17","ETSXB16P50EG7 / EPRA16DAW17","ETSXB16P30EG7 / EPRA16DAW17","ETSXB16P30EG7 / EPRA16DBW17","ETSXB16P50EG7 / EPRA16DBW17","ETSXB16P30EF7 / EPRA16DAW17","ETSXB16P50EF7 / EPRA16DAW17","ETSXB16P30EF7 / EPRA16DBW17","ETSXB16P50EF7 / EPRA16DBW17","ETSXB16P50EG7 / EPRA18DAW17","ETSXB16P30EG7 / EPRA18DAW17","ETSXB16P30EG7 / EPRA18DBW17","ETSXB16P50EG7 / EPRA18DBW17","ETSXB16P30EF7 / EPRA18DAW17","ETSXB16P50EF7 / EPRA18DAW17","ETSXB16P30EF7 / EPRA18DBW17","ETSXB16P50EF7 / EPRA18DBW17"]
["Heating capacity","Min.","","","kW","3.70 (1)","3.70 (1)","3.70 (1)","3.70 (1)","3.70 (1)","3.70 (1)","3.70 (1)","3.70 (1)","3.96 (1)","3.96 (1)","3.96 (1)","3.96 (1)","3.96 (1)","3.96 (1)","3.96 (1)","3.96 (1)","4.40 (1)","4.40 (1)","4.40 (1)","4.40 (1)","4.40 (1)","4.40 (1)","4.40 (1)","4.40 (1)"]
["","Nom.","","","kW","5.90 (2)","5.90 (2)","5.90 (2)","5.90 (2)","5.90 (2)","5.90 (2)","5.90 (2)","5.90 (2)","9.00 (2)","9.00 (2)","9.00 (2)","9.00 (2)","9.00 (2)","9.00 (2)","9.00 (2)","9.00 (2)","9.00 (2)","9.00 (2)","9.00 (2)","9.00 (2)","9.00 (2)","9.00 (2)","9.00 (2)","9.00 (2)"]
["","Max.","","","kW","9.75 (1)","9.75 (1)","9.75 (1)","9.75 (1)","9.75 (1)","9.75 (1)","9.75 (1)","9.75 (1)","10.44 (1)","10.44 (1)","10.44 (1)","10.44 (1)","10.44 (1)","10.44 (1)","10.44 (1)","10.44 (1)","11.60 (1)","11.60 (1)","11.60 (1)","11.60 (1)","11.60 (1)","11.60 (1)","11.60 (1)","11.60 (1)"]
["Cooling capacity","Nom.","","","kW","10.6 (3), 6.90 (4)","10.6 (3), 6.90 (4)","10.6 (3), 6.90 (4)","10.6 (3), 6.90 (4)","10.6 (3), 6.90 (4)","10.6 (3), 6.90 (4)","10.6 (3), 6.90 (4)","10.6 (3), 6.90 (4)","11.5 (3), 7.88 (4)","11.5 (3), 7.88 (4)","11.5 (3), 7.88 (4)","11.5 (3), 7.88 (4)","11.5 (3), 7.88 (4)","11.5 (3), 7.88 (4)","11.5 (3), 7.88 (4)","11.5 (3), 7.88 (4)","12.5 (3), 8.86 (4)","12.5 (3), 8.86 (4)","12.5 (3), 8.86 (4)","12.5 (3), 8.86 (4)","12.5 (3), 8.86 (4)","12.5 (3), 8.86 (4)","12.5 (3), 8.86 (4)","12.5 (3), 8.86 (4)"]
["Power input","Heating","","Min.","kW","0.84 (5)","0.84 (5)","0.84 (5)","0.84 (5)","0.84 (5)","0.84 (5)","0.84 (5)","0.84 (5)","0.90 (5)","0.90 (5)","0.90 (5)","0.90 (5)","0.90 (5)","0.90 (5)","0.90 (5)","0.90 (5)","1.00 (5)","1.00 (5)","1.00 (5)","1.00 (5)","1.00 (5)","1.00 (5)","1.00 (5)","1.00 (5)"]
["","","","Nom.","kW","1.23 (2)","1.23 (2)","1.23 (2)","1.23 (2)","1.23 (2)","1.23 (2)","1.23 (2)","1.23 (2)","1.80 (2)","1.80 (2)","1.80 (2)","1.80 (2)","1.80 (2)","1.80 (2)","1.80 (2)","1.80 (2)","1.80 (2)","1.80 (2)","1.80 (2)","1.80 (2)","1.80 (2)","1.80 (2)","1.80 (2)","1.80 (2)"]
["","","","Max.","kW","2.17 (5)","2.17 (5)","2.17 (5)","2.17 (5)","2.17 (5)","2.17 (5)","2.17 (5)","2.17 (5)","2.32 (5)","2.32 (5)","2.32 (5)","2.32 (5)","2.32 (5)","2.32 (5)","2.32 (5)","2.32 (5)","2.58 (5)","2.58 (5)","2.58 (5)","2.58 (5)","2.58 (5)","2.58 (5)","2.58 (5)","2.58 (5)"]
["","Cooling","","Nom.","kW","2.55 (3), 2.56 (4)","2.55 (3), 2.56 (4)","2.55 (3), 2.56 (4)","2.55 (3), 2.56 (4)","2.55 (3), 2.56 (4)","2.55 (3), 2.56 (4)","2.55 (3), 2.56 (4)","2.55 (3), 2.56 (4)","2.80 (3), 2.93 (4)","2.80 (3), 2.93 (4)","2.80 (3), 2.93 (4)","2.80 (3), 2.93 (4)","2.80 (3), 2.93 (4)","2.80 (3), 2.93 (4)","2.80 (3), 2.93 (4)","2.80 (3), 2.93 (4)","3.05 (3), 3.31 (4)","3.05 (3), 3.31 (4)","3.05 (3), 3.31 (4)","3.05 (3), 3.31 (4)","3.05 (3), 3.31 (4)","3.05 (3), 3.31 (4)","3.05 (3), 3.31 (4)","3.05 (3), 3.31 (4)"]
["COP","","","","","4.79 (2)","4.79 (2)","4.79 (2)","4.79 (2)","4.79 (2)","4.79 (2)","4.79 (2)","4.79 (2)","5.00 (2)","5.00 (2)","5.00 (2)","5.00 (2)","5.00 (2)","5.00 (2)","5.00 (2)","5.00 (2)","5.00 (2)","5.00 (2)","5.00 (2)","5.00 (2)","5.00 (2)","5.00 (2)","5.00 (2)","5.00 (2)"]
["EER","","","","","4.13 (3), 2.70 (4)","4.13 (3), 2.70 (4)","4.13 (3), 2.70 (4)","4.13 (3), 2.70 (4)","4.13 (3), 2.70 (4)","4.13 (3), 2.70 (4)","4.13 (3), 2.70 (4)","4.13 (3), 2.70 (4)","4.11 (3), 2.69 (4)","4.11 (3), 2.69 (4)","4.11 (3), 2.69 (4)","4.11 (3), 2.69 (4)","4.11 (3), 2.69 (4)","4.11 (3), 2.69 (4)","4.11 (3), 2.69 (4)","4.11 (3), 2.69 (4)","4.09 (3), 2.68 (4)","4.09 (3), 2.68 (4)","4.09 (3), 2.68 (4)","4.09 (3), 2.68 (4)","4.09 (3), 2.68 (4)","4.09 (3), 2.68 (4)","4.09 (3), 2.68 (4)","4.09 (3), 2.68 (4)"]
["Domestic hot water heating","General","","Declared load profile","","XL","L","L","XL","L","XL","L","XL","XL","L","L","XL","L","XL","L","XL","XL","L","L","XL","L","XL","L","XL"]
["","Average climate","","Water heating energy efficiency class","","A+","A+","A+","A+","A+","A+","A+","A+","A+","A+","A+","A+","A+","A+","A+","A+","A+","A+","A+","A+","A+","A+","A+","A+"]
["Space heating","Average climate water outlet 55°C","General","SCOP","","3.63","3.63","3.63","3.63","3.63","3.63","3.63","3.63","3.63","3.63","3.63","3.63","3.63","3.63","3.63","3.63","3.63","3.63","3.63","3.63","3.63","3.63","3.63","3.63"]
["","","","Seasonal space heating eff. class","","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++"]
["","Average climate water outlet 35°C","General","SCOP","","4.81","4.81","4.81","4.81","4.81","4.81","4.81","4.81","4.81","4.81","4.81","4.81","4.81","4.81","4.81","4.81","4.81","4.81","4.81","4.81","4.81","4.81","4.81","4.81"]
["","","","Seasonal space heating eff. class","","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++"]
["Energy Efficiency Range","","","","","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F"]
["Notes","","","","","(1) - Capacity according to standard EN14511 and valid for heated water range dT = 3~8°C at Ta 7°C","(1) - Capacity according to standard EN14511 and valid for heated water range dT = 3~8°C at Ta 7°C","(1) - Capacity according to standard EN14511 and valid for heated water range dT = 3~8°C at Ta 7°C","(1) - Capacity according to standard EN14511 and valid for heated water range dT = 3~8°C at Ta 7°C","(1) - Capacity according to standard EN14511 and valid for heated water range dT = 3~8°C at Ta 7°C","(1) - Capacity according to standard EN14511 and valid for heated water range dT = 3~8°C at Ta 7°C","(1) - Capacity according to standard EN14511 and valid for heated water range dT = 3~8°C at Ta 7°C","(1) - Capacity according to standard EN14511 and valid for heated water range dT = 3~8°C at Ta 7°C","(1) - Capacity according to standard EN14511 and valid for heated water range dT = 3~8°C at Ta 7°C","(1) - Capacity according to standard EN14511 and valid for heated water range dT = 3~8°C at Ta 7°C","(1) - Capacity according to standard EN14511 and valid for heated water range dT = 3~8°C at Ta 7°C","(1) - Capacity according to standard EN14511 and valid for heated water range dT = 3~8°C at Ta 7°C","(1) - Capacity according to standard EN14511 and valid for heated water range dT = 3~8°C at Ta 7°C","(1) - Capacity according to standard EN14511 and valid for heated water range dT = 3~8°C at Ta 7°C","(1) - Capacity according to standard EN14511 and valid for heated water range dT = 3~8°C at Ta 7°C","(1) - Capacity according to standard EN14511 and valid for heated water range dT = 3~8°C at Ta 7°C","(1) - Capacity according to standard EN14511 and valid for heated water range dT = 3~8°C at Ta 7°C","(1) - Capacity according to standard EN14511 and valid for heated water range dT = 3~8°C at Ta 7°C","(1) - Capacity according to standard EN14511 and valid for heated water range dT = 3~8°C at Ta 7°C","(1) - Capacity according to standard EN14511 and valid for heated water range dT = 3~8°C at Ta 7°C","(1) - Capacity according to standard EN14511 and valid for heated water range dT = 3~8°C at Ta 7°C","(1) - Capacity according to standard EN14511 and valid for heated water range dT = 3~8°C at Ta 7°C","(1) - Capacity according to standard EN14511 and valid for heated water range dT = 3~8°C at Ta 7°C","(1) - Capacity according to standard EN14511 and valid for heated water range dT = 3~8°C at Ta 7°C"]
["","","","","","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(3) - Cooling: EW 23°C; LW 18°C; ambient conditions: 35°CDB","(3) - Cooling: EW 23°C; LW 18°C; ambient conditions: 35°CDB","(3) - Cooling: EW 23°C; LW 18°C; ambient conditions: 35°CDB","(3) - Cooling: EW 23°C; LW 18°C; ambient conditions: 35°CDB","(3) - Cooling: EW 23°C; LW 18°C; ambient conditions: 35°CDB","(3) - Cooling: EW 23°C; LW 18°C; ambient conditions: 35°CDB","(3) - Cooling: EW 23°C; LW 18°C; ambient conditions: 35°CDB","(3) - Cooling: EW 23°C; LW 18°C; ambient conditions: 35°CDB","(3) - Cooling: EW 23°C; LW 18°C; ambient conditions: 35°CDB","(3) - Cooling: EW 23°C; LW 18°C; ambient conditions: 35°CDB","(3) - Cooling: EW 23°C; LW 18°C; ambient conditions: 35°CDB","(3) - Cooling: EW 23°C; LW 18°C; ambient conditions: 35°CDB","(3) - Cooling: EW 23°C; LW 18°C; ambient conditions: 35°CDB","(3) - Cooling: EW 23°C; LW 18°C; ambient conditions: 35°CDB","(3) - Cooling: EW 23°C; LW 18°C; ambient conditions: 35°CDB","(3) - Cooling: EW 23°C; LW 18°C; ambient conditions: 35°CDB","(3) - Cooling: EW 23°C; LW 18°C; ambient conditions: 35°CDB","(3) - Cooling: EW 23°C; LW 18°C; ambient conditions: 35°CDB","(3) - Cooling: EW 23°C; LW 18°C; ambient conditions: 35°CDB","(3) - Cooling: EW 23°C; LW 18°C; ambient conditions: 35°CDB","(3) - Cooling: EW 23°C; LW 18°C; ambient conditions: 35°CDB","(3) - Cooling: EW 23°C; LW 18°C; ambient conditions: 35°CDB","(3) - Cooling: EW 23°C; LW 18°C; ambient conditions: 35°CDB","(3) - Cooling: EW 23°C; LW 18°C; ambient conditions: 35°CDB"]
["","","","","","(4) - Cooling: EW 12°C; LW 7°C; ambient conditions: 35°CDB","(4) - Cooling: EW 12°C; LW 7°C; ambient conditions: 35°CDB","(4) - Cooling: EW 12°C; LW 7°C; ambient conditions: 35°CDB","(4) - Cooling: EW 12°C; LW 7°C; ambient conditions: 35°CDB","(4) - Cooling: EW 12°C; LW 7°C; ambient conditions: 35°CDB","(4) - Cooling: EW 12°C; LW 7°C; ambient conditions: 35°CDB","(4) - Cooling: EW 12°C; LW 7°C; ambient conditions: 35°CDB","(4) - Cooling: EW 12°C; LW 7°C; ambient conditions: 35°CDB","(4) - Cooling: EW 12°C; LW 7°C; ambient conditions: 35°CDB","(4) - Cooling: EW 12°C; LW 7°C; ambient conditions: 35°CDB","(4) - Cooling: EW 12°C; LW 7°C; ambient conditions: 35°CDB","(4) - Cooling: EW 12°C; LW 7°C; ambient conditions: 35°CDB","(4) - Cooling: EW 12°C; LW 7°C; ambient conditions: 35°CDB","(4) - Cooling: EW 12°C; LW 7°C; ambient conditions: 35°CDB","(4) - Cooling: EW 12°C; LW 7°C; ambient conditions: 35°CDB","(4) - Cooling: EW 12°C; LW 7°C; ambient conditions: 35°CDB","(4) - Cooling: EW 12°C; LW 7°C; ambient conditions: 35°CDB","(4) - Cooling: EW 12°C; LW 7°C; ambient conditions: 35°CDB","(4) - Cooling: EW 12°C; LW 7°C; ambient conditions: 35°CDB","(4) - Cooling: EW 12°C; LW 7°C; ambient conditions: 35°CDB","(4) - Cooling: EW 12°C; LW 7°C; ambient conditions: 35°CDB","(4) - Cooling: EW 12°C; LW 7°C; ambient conditions: 35°CDB","(4) - Cooling: EW 12°C; LW 7°C; ambient conditions: 35°CDB","(4) - Cooling: EW 12°C; LW 7°C; ambient conditions: 35°CDB"]
["","","","","","(5) - Power input is total input of indoor and outdoor units, including the circulation pump; according to EN14511","(5) - Power input is total input of indoor and outdoor units, including the circulation pump; according to EN14511","(5) - Power input is total input of indoor and outdoor units, including the circulation pump; according to EN14511","(5) - Power input is total input of indoor and outdoor units, including the circulation pump; according to EN14511","(5) - Power input is total input of indoor and outdoor units, including the circulation pump; according to EN14511","(5) - Power input is total input of indoor and outdoor units, including the circulation pump; according to EN14511","(5) - Power input is total input of indoor and outdoor units, including the circulation pump; according to EN14511","(5) - Power input is total input of indoor and outdoor units, including the circulation pump; according to EN14511","(5) - Power input is total input of indoor and outdoor units, including the circulation pump; according to EN14511","(5) - Power input is total input of indoor and outdoor units, including the circulation pump; according to EN14511","(5) - Power input is total input of indoor and outdoor units, including the circulation pump; according to EN14511","(5) - Power input is total input of indoor and outdoor units, including the circulation pump; according to EN14511","(5) - Power input is total input of indoor and outdoor units, including the circulation pump; according to EN14511","(5) - Power input is total input of indoor and outdoor units, including the circulation pump; according to EN14511","(5) - Power input is total input of indoor and outdoor units, including the circulation pump; according to EN14511","(5) - Power input is total input of indoor and outdoor units, including the circulation pump; according to EN14511","(5) - Power input is total input of indoor and outdoor units, including the circulation pump; according to EN14511","(5) - Power input is total input of indoor and outdoor units, including the circulation pump; according to EN14511","(5) - Power input is total input of indoor and outdoor units, including the circulation pump; according to EN14511","(5) - Power input is total input of indoor and outdoor units, including the circulation pump; according to EN14511","(5) - Power input is total input of indoor and outdoor units, including the circulation pump; according to EN14511","(5) - Power input is total input of indoor and outdoor units, including the circulation pump; according to EN14511","(5) - Power input is total input of indoor and outdoor units, including the circulation pump; according to EN14511","(5) - Power input is total input of indoor and outdoor units, including the circulation pump; according to EN14511"]