{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":34,"n_cols":14,"rows_kept":34,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FAA-B / RZAG-NV1"]
[]
[]
[]
[]
["","","","","FAA71BUV1B / RZAG71N2V1B","FAA71BUV1B / RZAG71N7V1B","FAA100BUV1B / RZAG71N2V1B","FAA100BUV1B / RZAG71N7V1B","FAA100BUV1B / RZAG100N2V1B","FAA100BUV1B / RZAG100N7V1B","FAA71BUV1B / FAA71BUV1B / RZAG100N2V1B","FAA71BUV1B / FAA71BUV1B / RZAG100N7V1B","FAA71BUV1B / FAA71BUV1B / RZAG140N2V1B","FAA71BUV1B / FAA71BUV1B / RZAG140N7V1B"]
["Cooling capacity","Nom.","","kW","6.80","6.80 (1)","","","9.50","9.50 (1)"]
["Space cooling","SEER","","","6.58","6.58","","","6.42","6.42"]
["","Annual energy consumption","","kWh/a","362","362","","","518","518"]
["","Capacity","Pdesign","kW","6.80","6.80","","","9.50","9.50"]
["","Energy efficiency class","","","A++","A++","","","A++","A++"]
["Space heating (Average climate)","Capacity","Pdesign","kW","4.70","4.70","","","7.80","7.80"]
["","SCOP/A","","","4.20","4.20","","","4.01","4.01"]
["","Energy efficiency class","","","A+","A+","","","A+","A+"]
["","Annual energy consumption","","kWh/a","1,567","1,567","","","2,725","2,723"]
["Nominal efficiency","EER","","","3.27","","","","3.24"]
["","Annual energy consumption","","kWh","1,040","","","","1,466"]
["","COP","","","3.42","","","","3.17"]
["","Energy labeling Directive","Cooling","","A","","","","A"]
["","","Heating","","B","","","","D"]
["Heating capacity","Nom.","","kW","7.50","7.50 (2)","","","10.80","10.8 (2)"]
["Notes","","","","","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["Cooling capacity","Nom.","","kW","","","6.80 (1)","6.80 (1)","","","9.50 (1)","9.50 (1)","13.4 (1)","13.4 (1)"]
["Heating capacity","Nom.","","kW","","","7.50 (2)","7.50 (2)","","","10.8 (2)","10.8 (2)","15.5 (2)","15.5 (2)"]
["Space cooling","Energy efficiency class","","","","","A++","A++","","","A+++","A+++"]
["","Capacity","Pdesign","kW","","","6.80","6.80","","","9.50","9.50","13.4","13.4"]
["","SEER","","","","","6.43","6.43","","","8.57","8.57","8.18","8.18"]
["","Annual energy consumption","","kWh/a","","","370","370","","","388","388","982","982"]
["Space heating (Average climate)","Energy efficiency class","","","","","A+","A+","","","A++","A++"]
["","Capacity","Pdesign","kW","","","4.70","4.70","","","7.80","7.80","9.52","9.52"]
["","SCOP/A","","","","","4.10","4.10","","","4.63","4.63","4.52","4.52"]
["","Annual energy consumption","","kWh/a","","","1605","1605","","","2359","2359","2946","2946"]
["Energy Efficiency Range","","","","","","A+++ ~ D","A+++ ~ D","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]