{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":7,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FAA-B / RZASG-MV1"]
[]
[]
[]
[]
["","","","","FAA100BUV1B / RZASG100M7V1B","FAA71BUV1B / RZASG71M2V1B","FAA71BUV1B / FAA71BUV1B / RZASG140M7V1B"]
["Cooling capacity","Nom.","","kW","","6.80 (1)"]
["Space cooling","SEER","","","","6.41"]
["","Annual energy consumption","","kWh/a","","371"]
["","Capacity","Pdesign","kW","","6.80"]
["","Energy efficiency class","","","","A++"]
["Space heating (Average climate)","Capacity","Pdesign","kW","","4.50"]
["","SCOP/A","","","","3.90"]
["","Energy efficiency class","","","","A"]
["","Annual energy consumption","","kWh/a","","1,615"]
["Heating capacity","Nom.","","kW","","7.50 (2)"]
["Cooling capacity","Nom.","","kW","9.5","","13.4"]
["Heating capacity","Nom.","","kW","10.8","","15.5"]
["Space cooling","Energy efficiency class","","","A+"]
["","Capacity","Pdesign","kW","9.5","","13.4"]
["","SEER","","","5.83","","8.15"]
["","Annual energy consumption","","kWh/a","570","","986"]
["Space heating (Average climate)","Energy efficiency class","","","A"]
["","Capacity","Pdesign","kW","6","","7.80"]
["","SCOP/A","","","3.85","","4.53"]
["","Annual energy consumption","","kWh/a","2182","","2409"]
["Notes","","","","","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","","(3) - See separate drawing for operation range"]
["","","","","","(4) - See separate drawing for electrical data"]