{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":6,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBA-A(9) / RXM-A9"]
[]
[]
[]
[]
["","","","","FBA35A2VEB9 / RXM35A5V1B9","FBA50A2VEB9 / RXM50A5V1B9"]
["Cooling capacity","Nom.","","kW","3.4","5"]
["Heating capacity","Nom.","","kW","4","5.5"]
["Nominal efficiency","EER","","","4.02","3.55"]
["","COP","","","4.02","3.83"]
["","Annual energy consumption","","kWh","423","704"]
["","Energy labeling Directive","Cooling","","A","A"]
["","","Heating","","A","A"]
["Space cooling","Energy efficiency class","","","A++","A++"]
["","Capacity","Pdesign","kW","3.4","5"]
["","SEER","","","6.3","6.27"]
["","Annual energy consumption","","kWh/a","189","279"]
["Space heating (Average climate)","Energy efficiency class","","","A+","A+"]
["","Capacity","Pdesign","kW","2.9","4.4"]
["","SCOP/A","","","4.17","4.06"]
["","Pdh Heating capacity at -10°","","kW","2.32","3.73"]
["","Annual energy consumption","","kWh/a","973","1517"]
["Energy Efficiency Range","","","","A+++ ~ D","A+++ ~ D"]
["Notes","","","","(1) - See separate drawing for operation range","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(2) - See separate drawing for electrical data","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(3) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(3) - See separate drawing for operation range"]
["","","","","(4) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(4) - See separate drawing for electrical data"]