{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":8,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBA-A(9) / RZQSG-L3/9V1"]
[]
[]
[]
[]
["","","","","FBA71A2VEB9 / RZQSG71L3V1B","FBA35A2VEB9 / FBA35A2VEB9 / FBA35A2VEB9 / RZQSG100L9V1B","FBA125A2VEB / RZQSG125L9V1B","FBA140A2VEB / RZQSG140L9V1B"]
["Cooling capacity","Nom.","","kW","6.80","9.50","12.00","13.40"]
["Space cooling","SEER","","","5.84","5.10","5.47","5.23"]
["","Annual energy consumption","","kWh/a","408","652","768","1,537"]
["","Capacity","Pdesign","kW","6.80","9.50","12.00","13.40"]
["","Energy efficiency class","","","A+","A","A"]
["Space heating (Average climate)","Capacity","Pdesign","kW","6.00","7.60","7.60","11.57"]
["","SCOP/A","","","4.01","3.80","4.01","3.81"]
["","Energy efficiency class","","","A+","A","A+"]
["","Annual energy consumption","","kWh/a","2,095","2,800","2,653","4,255"]
["Nominal efficiency","EER","","","3.43","3.28","3.23","2.28"]
["","Annual energy consumption","","kWh","991","","1,858"]
["","COP","","","3.92","","3.63","3.40"]
["","Energy labeling Directive","Cooling","","A","","A"]
["","","Heating","","A","","A"]
["Heating capacity","Nom.","","kW","7.50","","13.50","15.50"]
["Notes","","","","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range"]
["","","","","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data"]