{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":7,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBA-A / RZQSG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FBA35A2VEB / FBA35A2VEB / FBA35A2VEB / FBA35A2VEB / RZQSG125L8Y1B","FBA60A2VEB / FBA60A2VEB / RZQSG125L8Y1B","FBA35A2VEB / FBA35A2VEB / FBA35A2VEB / FBA35A2VEB / RZQSG140L7Y1B"]
["Cooling capacity","Nom.","","kW","12.0 (1)","12.0 (1)","13.4 (1)"]
["Space cooling","SEER","","","4.80","4.80"]
["","Annual energy consumption","","kWh/a","875","875"]
["","Capacity","Pdesign","kW","12.0","12.0"]
["","Energy efficiency class","","","B","B"]
["Space heating (Average climate)","Capacity","Pdesign","kW","7.60","7.60"]
["","SCOP/A","","","3.80","3.80"]
["","Energy efficiency class","","","A","A"]
["","Annual energy consumption","","kWh/a","2,800","2,800"]
["Nominal efficiency","EER","","","3.04 (3)","2.83 (3)","4.20 (3)"]
["","COP","","","3.35 (3)","3.26 (3)"]
["","Energy labeling Directive","Cooling","","B","C"]
["","","Heating","","C","C"]
["Heating capacity","Nom.","","kW","13.5 (2)","13.5 (2)","15.5 (2)"]
["Notes","","","","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 7.5m; level difference: 0m","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 7.5m; level difference: 0m","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 7.5m; level difference: 0m"]
["","","","","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 7.5m; level difference: 0m","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 7.5m; level difference: 0m","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 7.5m; level difference: 0m"]
["","","","","(3) - EER/COP according to Eurovent 2012, for use outside EU only","(3) - EER/COP according to Eurovent 2012, for use outside EU only","(3) - EER/COP according to Eurovent 2012, for use outside EU only"]