{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":17,"n_cols":6,"rows_kept":17,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDA-A / RZAG-NY1"]
[]
[]
[]
[]
["","","","","FDA125A5VEB / RZAG125N7Y1B","FDA125A5VEB / RZAG125N2Y1B"]
["Cooling capacity","Nom.","","kW","12.1 (1)","12.1 (1)"]
["Heating capacity","Nom.","","kW","13.5 (2)","13.5 (2)"]
["Space cooling","Capacity","Pdesign","kW","12.1","12.1"]
["","SEER","","","6.59","6.59"]
["","Annual energy consumption","","kWh/a","1102","1102"]
["Space heating (Average climate)","Capacity","Pdesign","kW","9.52","9.52"]
["","SCOP/A","","","4.35","4.35"]
["","Annual energy consumption","","kWh/a","3064","3064"]
["Energy Efficiency Range","","","","A+++ ~ D","A+++ ~ D"]
["Notes","","","","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]