{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":67,"n_cols":8,"rows_kept":67,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDA-A"]
[]
[]
[]
[]
["","","","","","FDA125A5VEB","FDA200AXVEB","FDA250AXVEB"]
["Cooling capacity","Total capacity","","Nom.","kW","12.10","19.00","22.00"]
["Heating capacity","Total capacity","","Nom.","kW","13.50","22.4","24.0"]
["Casing","Colour","","","","Unpainted","Unpainted","Unpainted"]
["","Material","","","","Galvanised steel","Galvanised steel plate","Galvanised steel plate"]
["Dimensions","Unit","","Height","mm","300","470","470"]
["","","","Width","mm","1,400","1,490","1,490"]
["","","","Depth","mm","700","1,100","1,100"]
["Weight","Unit","","","kg","45","104","115"]
["Required ceiling void >","mm","","","","350"]
["Fan","Air flow rate","Cooling","High","m³/min","39.0","64.0","69.0"]
["","","","Medium","m³/min","","50","56"]
["","","","Low","m³/min","28.0","36.0","43.0"]
["","","Heating","High","m³/min","39.0","64.0","69.0"]
["","","","Medium","m³/min","","50.0","56.0"]
["","","","Low","m³/min","28.0","36.0","43.0"]
["","External static pressure","","High","Pa","200","250","250"]
["","","","Nom.","Pa","50","62","62"]
["Sound power level","Cooling","","","dBA","66","69.0","71.0"]
["Sound pressure level","Cooling","","High","dBA","40","43.0","44.0"]
["","","","Medium","dBA","","39.0","40.0"]
["","","","Low","dBA","33","36.0","37.0"]
["","Heating","","High","dBA","40","43.0","44.0"]
["","","","Medium","dBA","","39.0","40.0"]
["","","","Low","dBA","33","36.0","37.0"]
["Piping connections","Liquid","","OD","mm","9.52","9.52","9.52"]
["","Gas","","OD","mm","15.90","19.1","22.2"]
["","Drain","","","","VP25 (I.D. 25/O.D. 32)","BSP1","BSP1"]
["Drain-up height","mm","","","","625"]
["Decoration panel","Model","","","","BYBS125DJW1"]
["","Colour","","","","White (10Y9/0.5)"]
["","Dimensions","","Height","mm","55"]
["","","","Width","mm","1,500"]
["","","","Depth","mm","500"]
["","Weight","","","kg","6.5"]
["Control systems","Infrared remote control","","","","BRC4C65, BRC4C66"]
["","Wired remote control","","","","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["Standard Accessories","Screws","","","","16","2","2"]
["","Washer","","","","8","12","12"]
["","Hose band","","","","1"]
["","Drain hose","","","","1"]
["","General safety precautions","","","","1","1","1"]
["","Installation and operation manual","","","","1","1","1"]
["","Wire for common power supply","","","","2"]
["","Sealing material (drain hose)","","","","1"]
["","Sealing material","","","","2"]
["","Thermal insulation tube (liquid)","","","","1"]
["","Thermal insulation tube (gas)","","","","1"]
["Power supply","Name","","","","","VE","VE"]
["","Phase","","","","1~","1~","1~"]
["","Frequency","","","Hz","50/60","50/60","50/60"]
["","Voltage","","","V","220-240/220","220-240/220","220-240/220"]
["Notes","","","","","(1) - See separate drawing for electrical data"]
["Standard Accessories","Operation manual","","","","","1","1"]
["","Installation manual","","","","","1","1"]
["","Gas connection pipe","","","","","1","1"]
["","Wire clamp material","","","","","1","1"]
["","Spring washer","","","","","2","2"]
["","Screw+Washer","","","","","45","45"]
["","Hexagon head screw with washer","","","","","49","49"]
["","Hexagon head screw","","","","","2","2"]
["","Plain washer","","","","","8","8"]