{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":5,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDQ-B / RQ-BW1"]
[]
[]
[]
[]
["","","","","FDQ125B8V3B9 / RQ125B8W1B"]
["Cooling capacity","Nom.","","kW","12.5 (6)"]
["Piping connections","Liquid","OD","mm","9.52"]
["","Gas","OD","mm","15.9"]
["","Drain","OD","mm","26"]
["Nominal efficiency","EER","","","2.61"]
["","Annual energy consumption","","kWh","2,395"]
["","COP","","","3.24"]
["","Energy labeling Directive","Cooling","","D"]
["","","Heating","","C"]
["Heating capacity","Nom.","","kW","14.6 (7)"]
["Notes","","","","(1) - Sound pressure level is a relative value, depending on the distance and acoustic environment. For more details, please refer to the sound level drawings."]
["","","","","(2) - The sound power level is an absolute value indicating the power which a sound source generates."]
["","","","","(3) - Sound values are measured in a semi-anechoic room."]
["","","","","(4) - Heating capacity is only applicable for combination with heat pump outdoor unit"]
["","","","","(5) - In case of drain piping for the outdoor unit, a drain piping kit (option) is needed."]
["","","","","(6) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 7.5m; level difference: 0m"]
["","","","","(7) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 7.5m; level difference: 0m"]
["","","","","(8) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load"]