{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":16,"n_cols":5,"rows_kept":16,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDQ-B / RZQS-DV1"]
[]
[]
[]
[]
["","","","","FDQ125B8V3B9 / RZQS125D7V1B"]
["Cooling capacity","Nom.","","kW","12.5 (1)"]
["Nominal efficiency","EER","","","2.91"]
["","Annual energy consumption","","kWh","2,148"]
["","COP","","","3.53"]
["","Energy labeling Directive","Cooling","","C"]
["","","Heating","","B"]
["Heating capacity","Nom.","","kW","14 (2)"]
["Notes","","","","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m; level difference: 0m"]
["","","","","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m; level difference: 0m"]
["","","","","(3) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load"]