{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":21,"n_cols":11,"rows_kept":21,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F9 / RZASG-MV"]
[]
[]
[]
[]
["","","","","FDXM35F3V1B9 / FDXM35F3V1B9 / FDXM35F3V1B9 / RZASG100MUV","FDXM50F3V1B9 / FDXM50F3V1B9 / RZASG100MUV","FDXM35F3V1B9 / FDXM35F3V1B9 / FDXM35F3V1B9 / FDXM35F3V1B9 / RZASG125MUV","FDXM50F3V1B9 / FDXM50F3V1B9 / FDXM50F3V1B9 / RZASG125MUV","FDXM60F3V1B9 / FDXM60F3V1B9 / RZASG125MUV","FDXM35F3V1B9 / FDXM35F3V1B9 / FDXM35F3V1B9 / FDXM35F3V1B9 / RZASG140MUV","FDXM50F3V1B9 / FDXM50F3V1B9 / FDXM50F3V1B9 / RZASG140MUV"]
["Cooling capacity","Nom.","","kW","9.50 (1)","9.50 (1)","12.1 (1)","12.1 (1)","12.1 (1)","13.4 (1)","13.4 (1)"]
["Heating capacity","Nom.","","kW","10.8 (2)","10.8 (2)","13.5 (2)","13.5 (2)","13.5 (2)","15.5 (2)","15.5 (2)"]
["Space cooling","Energy efficiency class","","","A++","A++"]
["","Capacity","Pdesign","kW","9.50","9.50","12.1","12.1","12.1","13.4","13.4"]
["","SEER","","","6.43","7.68","6.69","7.00","6.46","6.74","8.57"]
["","Annual energy consumption","","kWh/a","517","433","1086","1037","1124","1194","939"]
["Space heating (Average climate)","Energy efficiency class","","","A","A"]
["","Capacity","Pdesign","kW","6.00","6.00","6.00","6.00","6.00","7.80","7.80"]
["","SCOP/A","","","3.89","3.93","4.39","4.42","4.07","4.57","4.56"]
["","Annual energy consumption","","kWh/a","2159","2137","1912","1900","2065","2387","2394"]
["Energy Efficiency Range","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Notes","","","","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range"]
["","","","","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data"]