{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":47,"n_cols":9,"rows_kept":47,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F9"]
[]
[]
[]
[]
["","","","","","FDXM25F3V1B9","FDXM35F3V1B9","FDXM50F3V1B9","FDXM60F3V1B9"]
["Power input","Cooling","","Nom.","kW","0.036","0.036","0.060","0.060"]
["","Heating","","Nom.","kW","0.036","0.036","0.060","0.060"]
["Dimensions","Unit","","Height","mm","200","200","200","200"]
["","","","Width","mm","750","750","1150","1150"]
["","","","Depth","mm","620","620","620","620"]
["Weight","Unit","","","kg","21","21","28","28"]
["Fan","Air flow rate","Cooling","High","m³/min","8.7","8.7","15.8","16.0"]
["","","","Medium","m³/min","8.0","8.0","14.6","14.8"]
["","","","Low","m³/min","7.3","7.3","13.3","13.5"]
["","","Heating","High","m³/min","8.7","8.7","15.8","16.0"]
["","","","Medium","m³/min","8.0","8.0","14.6","14.8"]
["","","","Low","m³/min","7.3","7.3","13.3","13.5"]
["","External static pressure","","Nom.","Pa","30","30","40","40"]
["Sound power level","Cooling","","","dBA","53.0","53.0","55.0","56.0"]
["","Heating","","","dBA","53.0","53.0","55.0","56.0"]
["Sound pressure level","Cooling","","High","dBA","35.0","35.0","38.0","38.0"]
["","","","Medium","dBA","33.0","33.0","35.0","35.0"]
["","","","Low","dBA","27.0","27.0","30.0","30.0"]
["","Heating","","High","dBA","35.0","35.0","38.0","38.0"]
["","","","Medium","dBA","33.0","33.0","35.0","35.0"]
["","","","Low","dBA","27.0","27.0","30.0","30.0"]
["Piping connections","Liquid","","OD","mm","6.35","6.35","6.35","6.35"]
["","Gas","","OD","mm","9.50","9.50","12.70","12.70"]
["","Drain","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Standard Accessories","Installation manual","","","","1","1","1","1"]
["","Washer for hanger bracket","","","","8","8","8","8"]
["","Operation manual","","","","1","1","1","1"]
["","Clamp metal","","","","1","1","1","1"]
["","Clamps","","","","6","6","6","6"]
["","Drain hose","","","","1","1","1","1"]
["","Air filter","","","","1","1","1","1"]
["","Insulation for fitting","","","","1","1","1","1"]
["","Screws for duct flanges","","","","1","1","1","1"]
["","Sealing material","","","","2","2","2","2"]
["","Sealing pad","","","","1","1","1","1"]
["","Washer fixing plate","","","","4","4","4","4"]
["Energy Efficiency Range","","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Power supply","Phase","","","","1~","1~","1~","1~"]
["","Frequency","","","Hz","50","50","50","50"]
["","Voltage","","","V","220-240","220-240","220-240","220-240"]
["Notes","","","","","(1) - See separate drawing for electrical data","(1) - See separate drawing for electrical data","(1) - See separate drawing for electrical data","(1) - See separate drawing for electrical data"]