{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":6,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXS-F / RXS-L"]
[]
[]
[]
[]
["","","","","FDXS35F2VEB / RXS35L2V1B","FDXS60F2VEB / RXS60L2V1B"]
["Cooling capacity","Min.","","kW","1.4","1.7"]
["","Max.","","kW","3.8","6.5"]
["","Nom.","","kW","3.4","6.0"]
["Space cooling","SEER","","","5.21","5.51"]
["","Annual energy consumption","","kWh/a","228","381"]
["","Capacity","Pdesign","kW","3.40","6.00"]
["","Energy efficiency class","","","A","A"]
["Space heating (Average climate)","Capacity","Pdesign","kW","2.90","4.60"]
["","SCOP/A","","","3.88","3.80"]
["","Energy efficiency class","","","A","A"]
["","Annual energy consumption","","kWh/a","1,047","1,693"]
["Piping connections","Liquid","OD","mm","6.35","6.35"]
["","Gas","OD","mm","9.5","12.7"]
["","Drain","OD","mm","VP20 (External dia.26, Internal dia. 20)","VP20 (External dia.26, Internal dia. 20)"]
["Nominal efficiency","Annual energy consumption","","kWh","530","1,030"]
["","EER","","","3.21","2.91"]
["","COP","","","3.48","3.21"]
["","Energy labeling Directive","Cooling","","A","C"]
["","","Heating","","B","C"]
["Heating capacity","Nom.","","kW","4.0","7.0"]
["","Min.","","kW","1.4","1.7"]
["","Max.","","kW","5.0","8.0"]
["Notes","","","","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only"]
["","","","","(2) - 230V","(2) - 230V"]
["","","","","(3) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(3) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load"]