{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":17,"n_cols":7,"rows_kept":17,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHA-A / RZQSG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FHA35AVEB / FHA35AVEB / FHA35AVEB / RZQSG100L8Y1B","FHA50AVEB / FHA50AVEB / RZQSG100L8Y1B","FHA35AVEB / FHA35AVEB / FHA35AVEB / FHA35AVEB / RZQSG125L8Y1B"]
["Space cooling","Annual energy consumption","","kWh/a","652","652","875"]
["","Capacity","Pdesign","kW","9.50","9.50","12.0"]
["Space heating (Average climate)","Capacity","Pdesign","kW","7.60","7.60","7.60"]
["","Annual energy consumption","","kWh/a","2,800","2,800","2,800"]
["Space cooling","SEER","","","5.10","5.10","4.80"]
["","Energy efficiency class","","","A","A","B"]
["Space heating (Average climate)","SCOP/A","","","3.80","3.80","3.80"]
["","Energy efficiency class","","","A","A","A"]
["Notes","","","","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 7.5m; level difference: 0m","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 7.5m; level difference: 0m","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 7.5m; level difference: 0m"]
["","","","","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 7.5m; level difference: 0m","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 7.5m; level difference: 0m","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 7.5m; level difference: 0m"]
["","","","","(3) - EER/COP according to Eurovent 2012, for use outside EU only","(3) - EER/COP according to Eurovent 2012, for use outside EU only","(3) - EER/COP according to Eurovent 2012, for use outside EU only"]