{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":32,"n_cols":6,"rows_kept":32,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXL-JV / RXL-M"]
[]
[]
[]
[]
["","","","","FTXL25J2V1B / RXL25M2V1B","FTXL35J2V1B / RXL35M2V1B"]
["Cooling capacity","Min.","","kW","1.2","1.3"]
["","Max.","","kW","3.4","3.8"]
["Space cooling","SEER","","","6.01","5.87"]
["","Annual energy consumption","","kWh/a","146","209"]
["","Capacity","Pdesign","kW","2.50","3.50"]
["","Energy efficiency class","","","A+","A+"]
["Space heating (Average climate)","Capacity","Pdesign","kW","2.50","3.00"]
["","SCOP/A","","","4.37","4.21"]
["","Energy efficiency class","","","A+","A+"]
["","Annual energy consumption","","kWh/a","793","998"]
["Piping connections","Liquid","OD","mm","6.35","6.35"]
["","Gas","OD","mm","9.5","9.5"]
["","Drain","OD","mm","18","18"]
["Nominal efficiency","EER","","","3.12","3.07"]
["","Annual energy consumption","","kWh","400.5","570"]
["","COP","","","4.43","4.21"]
["","Energy labeling Directive","Cooling","","B","B"]
["","","Heating","","A","A"]
["Heating capacity","Min.","","kW","1.1","1.2"]
["","Max.","","kW","5.5","6.0"]
["Notes","","","","(1) - For rated minimal heating capacity indoor unit fan set to SL tap","(1) - For rated minimal heating capacity indoor unit fan set to SL tap"]
["","","","","(2) - 220V","(2) - 220V"]
["","","","","(3) - 230V","(3) - 230V"]
["","","","","(4) - 240V","(4) - 240V"]
["","","","","(5) - EER/COP according to Eurovent 2012, for use outside EU only","(5) - EER/COP according to Eurovent 2012, for use outside EU only"]
["","","","","(6) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(6) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load"]