{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":35,"n_cols":6,"rows_kept":35,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXLS-K / RXLS-M"]
[]
[]
[]
[]
["","","","","FTXLS25K2V1B / RXLS25M2V1B","FTXLS35K2V1B / RXLS35M2V1B"]
["Cooling capacity","Min.","","kW","1.6","1.7"]
["","Max.","","kW","4.4","5.0"]
["","Nom.","","kW","2.5","3.5"]
["Space cooling","SEER","","","6.62","6.91"]
["","Annual energy consumption","","kWh/a","132","177"]
["","Capacity","Pdesign","kW","2.50","3.50"]
["","Energy efficiency class","","","A++","A++"]
["Space heating (Average climate)","Capacity","Pdesign","kW","3.20","3.80"]
["","SCOP/A","","","4.62","4.60"]
["","Energy efficiency class","","","A++","A++"]
["","Annual energy consumption","","kWh/a","947","1,147"]
["Piping connections","Liquid","OD","mm","6.35","6.35"]
["","Gas","OD","mm","9.5","9.5"]
["","Drain","OD","mm","18","18"]
["Nominal efficiency","EER","","","3.74","3.69"]
["","Annual energy consumption","","kWh","334.5","475.5"]
["","COP","","","4.27","4.12"]
["","Energy labeling Directive","Cooling","","A","A"]
["","","Heating","","A","A"]
["Heating capacity","Nom.","","kW","4.7","5.4"]
["","Min.","","kW","1.0","1.0"]
["","Max.","","kW","6.6, 3.98 (7)","7.2, 4.51 (7)"]
["Notes","","","","(1) - For rated minimal heating capacity indoor unit fan set to SL tap","(1) - For rated minimal heating capacity indoor unit fan set to SL tap"]
["","","","","(2) - 220V","(2) - 220V"]
["","","","","(3) - 230V","(3) - 230V"]
["","","","","(4) - 240V","(4) - 240V"]
["","","","","(5) - EER/COP according to Eurovent 2012, for use outside EU only","(5) - EER/COP according to Eurovent 2012, for use outside EU only"]
["","","","","(6) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(6) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load"]
["","","","","(7) - Maximum heating capacity at -15°C outdoor temperature","(7) - Maximum heating capacity at -15°C outdoor temperature"]