{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":39,"n_cols":9,"rows_kept":39,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVXG-K / RXG-K"]
[]
[]
[]
[]
["","","","","FVXG25K2V1B / RXG25K2V1B","FVXG25K2V1B / RXG25K3V1B","FVXG35K2V1B / RXG35K2V1B","FVXG50K2V1B / RXG50K2V1B","FVXG50K2V1B / RXG50K3V1B"]
["Cooling capacity","Min.","","kW","1.3","1.3","1.4","1.7","1.7"]
["","Max.","","kW","3.0","3.0","3.8","5.6","5.6"]
["","Nom.","","kW","2.5 (3)","2.5 (2)","3.5 (3)","5.0 (3)","5.0 (2)"]
["Space cooling","SEER","","","","6.46","","","5.31"]
["","Annual energy consumption","","kWh/a","","135","","","330"]
["","Capacity","Pdesign","kW","","2.50","","","5.00"]
["","Energy efficiency class","","","","A++","","","A"]
["Space heating (Average climate)","Capacity","Pdesign","kW","","2.80","","","4.60"]
["","SCOP/A","","","","4.56","","","4.13"]
["","Energy efficiency class","","","","A+","","","A+"]
["","Annual energy consumption","","kWh/a","","858","","","1,559"]
["Piping connections","Liquid","OD","mm","6.35","6.35","6.35","6.35","6.35"]
["","Gas","OD","mm","9.5","9.5","9.5","12.7","12.7"]
["","Drain","OD","mm","18","18","18","18","18"]
["Nominal efficiency","EER","","","4.55","4.55","3.68","3.29","3.29"]
["","Annual energy consumption","","kWh","275","275","475","760","760"]
["","COP","","","4.36","4.36","3.72","3.67","3.67"]
["","Energy labeling Directive","Cooling","","A","A","A","A","A"]
["","","Heating","","A","A","A","A","A"]
["Heating capacity","Nom.","","kW","3.4 (4)","3.4 (3)","4.5 (4)","5.8 (4)","5.8 (3)"]
["","Min.","","kW","1.3","1.3","1.4","1.7","1.7"]
["","Max.","","kW","4.5","4.5","5.0","8.1","8.1"]
["Notes","","","","(1) - Energy label: scale from A (most efficient) to G (less efficient)","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - Energy label: scale from A (most efficient) to G (less efficient)","(1) - Energy label: scale from A (most efficient) to G (less efficient)","(1) - EER/COP according to Eurovent 2012, for use outside EU only"]
["","","","","(2) - Annual energy consumption: based on average use of 500 running hours per year at full load (nominal conditions)","(2) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB, 24°CWB","(2) - Annual energy consumption: based on average use of 500 running hours per year at full load (nominal conditions)","(2) - Annual energy consumption: based on average use of 500 running hours per year at full load (nominal conditions)","(2) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB, 24°CWB"]
["","","","","(3) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB, 24°CWB","(3) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB","(3) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB, 24°CWB","(3) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB, 24°CWB","(3) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB"]
["","","","","(4) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB, 24°CWB","(4) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB","(4) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB, 24°CWB","(4) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB, 24°CWB","(4) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB"]
["","","","","(5) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB","(5) - 220V","(5) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB","(5) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB","(5) - 220V"]
["","","","","(6) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB","(6) - 230V","(6) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB","(6) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB","(6) - 230V"]
["","","","","(7) - 220V","(7) - 240V","(7) - 220V","(7) - 220V","(7) - 240V"]
["","","","","(8) - 230V","(8) - When connected with multi-system outdoor unit, refer to the specifications of the multi outdoor unit to be connected.","(8) - 230V","(8) - 230V","(8) - When connected with multi-system outdoor unit, refer to the specifications of the multi outdoor unit to be connected."]
["","","","","(9) - 240V","(9) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(9) - 240V","(9) - 240V","(9) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load"]
["","","","","(10) - When connected with multi-system outdoor unit, refer to the specifications of the multi outdoor unit to be connected.","","(10) - When connected with multi-system outdoor unit, refer to the specifications of the multi outdoor unit to be connected.","(10) - When connected with multi-system outdoor unit, refer to the specifications of the multi outdoor unit to be connected."]
["","","","","(11) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","","(11) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(11) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load"]