{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":7,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FXMQ-A"]
[]
[]
[]
[]
["","","","","","FXMQ200AXVMB","FXMQ250AXVMB"]
["Cooling capacity","Total capacity","","At high fan speed","kW","22.4","28.0"]
["Heating capacity","Total capacity","","At high fan speed","kW","25.0","31.5"]
["Power input - 50Hz","Cooling","","At high fan speed","kW","0.54","0.65"]
["","Heating","","At high fan speed","kW","0.54","0.65"]
["Dimensions","Unit","","Height","mm","470","470"]
["","","","Width","mm","1490","1490"]
["","","","Depth","mm","1100","1100"]
["Weight","Unit","","","kg","105","115"]
["Casing","Colour","","","","Unpainted","Unpainted"]
["","Material","","","","Galvanised steel plate","Galvanised steel plate"]
["Fan","Air flow rate - 50Hz","Cooling","At high fan speed","m³/min","62","74"]
["","","","At low fan speed","m³/min","41","52"]
["","External static pressure - 50Hz","","High","Pa","250","250"]
["","","","Low","Pa","50","50"]
["","External static pressure - 60Hz","","High","Pa","250","250"]
["","","","Low","Pa","50","50"]
["Refrigerant","Type","","","","R-410A","R-410A"]
["","GWP","","","","2087.5","2087.5"]
["Sound power level","Cooling","","At high fan speed","dBA","75.0","76.0"]
["Sound pressure level","Cooling","","At high fan speed","dBA","48.0","48.0"]
["","","","At medium fan speed","dBA","46.5","46.5"]
["","","","At low fan speed","dBA","45.0","45.0"]
["","Heating","","At high fan speed","dBA","48.0","48.0"]
["","","","At medium fan speed","dBA","46.5","46.5"]
["","","","At low fan speed","dBA","45.0","45.0"]
["Piping connections","Liquid","","Type","","Flare connection","Flare connection"]
["","","","OD","mm","9.5","9.5"]
["","Gas","","Type","","Flange","Flange"]
["","","","OD","mm","19.1","22.2"]
["","Drain","","","","BSP1","BSP1"]
["Standard Accessories","General safety precautions","","","","1","1"]
["","Wire clamp material","","","","1","1"]
["","Spring washer","","","","2","2"]
["","Hexagon head screw","","","","2","2"]
["","Plain washer","","","","8","8"]
["","Hexagon head screw with washer","","","","49","49"]
["","Gas connection pipe","","","","1","1"]
["","Installation and operation manual","","","","1","1"]
["Power supply","Name","","","","VM","VM"]
["","Phase","","","","1~","1~"]
["","Frequency","","","Hz","50/60","50/60"]
["","Voltage","","","V","220-240/220-230","220-240/220-230"]
["Current - 50Hz","Maximum fuse amps (MFA)","","","A","6","6"]