{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":40,"n_cols":16,"rows_kept":40,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXM-A"]
[]
[]
[]
[]
["","","","","","RXM60A2V1B","RXM60A5V1B","RXM71A2V1B","RXM71A5V1B","RXM20A5V1B (Archived)","RXM25A5V1B (Archived)","RXM35A5V1B (Archived)","RXM42A2V1B (Archived)","RXM42A5V1B (Archived)","RXM50A2V1B (Archived)","RXM50A5V1B (Archived)"]
["Dimensions","Unit","","Height","mm","","734","","734","610","610","610","","610","","734"]
["","","","Width","mm","","954","","954","923","923","923","","923","","954"]
["","","","Depth","mm","","401","","401","367","367","367","","367","","401"]
["Weight","Unit","","","kg","","49","","55","36","36","36","","40","","49"]
["Fan motor","Speed","Cooling","Super low","rpm","","","","","600","600","600","","600","","500"]
["Compressor","Type","","","","","Hermetically sealed swing compressor","","Hermetically sealed swing compressor","Hermetically sealed swing compressor","Hermetically sealed swing compressor","Hermetically sealed swing compressor","","Hermetically sealed swing compressor","","Hermetically sealed swing compressor"]
["Operation range","Cooling","Ambient","Min.","°CDB","","-10","","-10","-10","-10","-10","","-10","","-10"]
["","","","Max.","°CDB","","50","","46","50","50","50","","50","","50 (1)"]
["","Heating","Ambient","Min.","°CWB","","-21","","-15","-21","-21","-21","","-21","","-21 (1)"]
["","","","Max.","°CWB","","18","","18","18","18","18","","18","","18"]
["Sound pressure level","Cooling","","Nom.","dBA","","48","","47","46","46","47","","48","","48"]
["","Heating","","Nom.","dBA","","49","","48","47","47","49","","49","","49"]
["Refrigerant","Type","","","","","R-32","","R-32","R-32","R-32","R-32","","R-32","","R-32"]
["","Charge","","","kg","","1.15","","1.15","0.95","0.95","0.95","","0.95","","1.10"]
["","Charge","","","tCO2Eq","","0.78","","0.78","0.65","0.65","0.65","","0.65","","0.75"]
["","GWP","","","","","675","","675","675","675","675","","675","","675"]
["Piping connections","Piping length","OU - IU","Max.","m","","30","","30","20","20","20","","30","","30"]
["","Additional refrigerant charge","","","kg/m","","0.02 (for piping length exceeding 10m)","","0.02 (for piping length exceeding 10m)","0.02 (for piping length exceeding 10m)","0.02 (for piping length exceeding 10m)","0.02 (for piping length exceeding 10m)","","0.02 (for piping length exceeding 10m)","","0.02 (for piping length exceeding 10m)"]
["","Level difference","IU - OU","Max.","m","","20","","20","15","15","15","","20","","20"]
["Energy Efficiency Range","","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Power supply","Phase","","","","","1~","","1~","1~","1~","1~","","1~","","1~"]
["","Frequency","","","Hz","","50","","50","50","50","50","","50","","50"]
["","Voltage","","","V","","220-240","","220-240","220-240","220-240","220-240","","220-240","","220-240"]
["Standard Accessories","Installation manual","","","","","1","","1","1","1","1","","1","","1"]
["","Refrigerant charge label","","","","","1","","1","1","1","1","","1","","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","","1","","1","1","1","1","","1","","1"]
["","Drain cap","","","","","3","","3","3","3","3","","3","","1"]
["","Drain plug","","","","","1","","1"]
["Notes","","","","","","(1) - See separate drawing for operation range","","(1) - See separate drawing for operation range","(1) - See separate drawing for operation range","(1) - See separate drawing for operation range","(1) - See separate drawing for operation range","","(1) - See separate drawing for operation range","","(1) - See separate drawing for operation range"]
["","","","","","","(2) - See separate drawing for electrical data","","(2) - See separate drawing for electrical data","(2) - See separate drawing for electrical data","(2) - See separate drawing for electrical data","(2) - See separate drawing for electrical data","","(2) - See separate drawing for electrical data","","(2) - See separate drawing for electrical data"]
["","","","","","","(3) - Contains fluorinated greenhouse gases","","(3) - Contains fluorinated greenhouse gases","(3) - Contains fluorinated greenhouse gases","(3) - Contains fluorinated greenhouse gases","(3) - Contains fluorinated greenhouse gases","","(3) - Contains fluorinated greenhouse gases","","(3) - Contains fluorinated greenhouse gases"]
["Standard Accessories","Drain joint","","","","","","","","1","1","1","","1","","1"]
["","General safety precautions","","","","","","","","1","1","1","","1","","1"]
["","LOT10 Energy Label","","","","","","","","1","1","1","","1","","1"]