{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":66,"n_cols":12,"rows_kept":66,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXYCQ-A"]
[]
[]
[]
[]
["","","","","","RXYCQ8A7Y1B","RXYCQ10A7Y1B","RXYCQ12A7Y1B","RXYCQ14A7Y1B","RXYCQ16A7Y1B","RXYCQ18A7Y1B","RXYCQ20A7Y1B"]
["Sound pressure level","Cooling","","Nom.","dBA","58","59","61","61","64","65","66"]
["Standard Accessories","Installation manual","","","","1","1","1","1","1","1","1"]
["","Operation manual","","","","1","1","1","1","1","1","1"]
["","Connection pipes","","","","4","4","4","4","4","4","4"]
["Capacity range","HP","","","","8","10","12","14","16","18","20"]
["Operation range","Cooling","","Max.","°CDB","43","43","43","43","43","43","43"]
["","","","Min.","°CDB","-5","-5","-5","-5","-5","-5","-5"]
["","Heating","","Min.","°CWB","-20","-20","-20","-20","-20","-20","-20"]
["","","","Max.","°CWB","15.5","15.5","15.5","15.5","15.5","15.5","15.5"]
["Maximum number of connectable indoor units","","","","","64","64","64","64","64","64","64"]
["Compressor","Type","","","","Hermetically sealed scroll compressor","Hermetically sealed scroll compressor","Hermetically sealed scroll compressor","Hermetically sealed scroll compressor","Hermetically sealed scroll compressor","Hermetically sealed scroll compressor","Hermetically sealed scroll compressor"]
["Weight","Unit","","","kg","159","187","240","240","316","316","324"]
["Refrigerant","Charge","","","TCO2Eq","12.9","16.1","17.5","18","23.6","24","24.4"]
["","GWP","","","","2,087.5","2,087.5","2,087.5","2,087.5","2,087.5","2,087.5","2,087.5"]
["","Charge","","","kg","6.2","7.7","8.4","8.6","11.3","11.5","11.7"]
["","Type","","","","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A"]
["Indoor index connection","Nom.","","","","200","250","300","350","400","450","500"]
["","Min.","","","","100","125","150","175","200","225","250"]
["","Max.","","","","200","250","360","420","480","540","600"]
["Piping connections","Liquid","","OD","mm","9.52","9.52","9.52","12.7","12.7","12.7","15.9"]
["","","","Type","","Braze connection","Braze connection","Braze connection","Braze connection","Braze connection","Braze connection","Braze connection"]
["","Total piping length","System","Actual","m","300","300","300","300","300","300","300"]
["","Gas","","OD","mm","15.9","19.1","22.2","28.6","28.6","28.6","28.6"]
["","","","Type","","Braze connection","Braze connection","Braze connection","Braze connection","Braze connection","Braze connection","Braze connection"]
["","Level difference","OU - IU","Outdoor unit in highest position","m","30","30","30","30","30","30","30"]
["","","IU - IU","Max.","m","15","15","15","15","15","15","15"]
["","Heat insulation","","","","Both liquid and gas pipes","Both liquid and gas pipes","Both liquid and gas pipes","Both liquid and gas pipes","Both liquid and gas pipes","Both liquid and gas pipes","Both liquid and gas pipes"]
["Sound power level","Cooling","","Nom.","dBA","78","81","81","81","86","86","88"]
["Dimensions","Unit","","Width","mm","635","930","930","930","1,240","1,240","1,240"]
["","","","Depth","mm","765","765","765","765","765","765","765"]
["","","","Height","mm","1,680","1,680","1,680","1,680","1,680","1,680","1,680"]
["Fan","External static pressure","","Max.","Pa","78","78","78","78","78","78","78"]
["Power supply","Phase","","","","3N~","3N~","3N~","3N~","3N~","3N~","3N~"]
["","Name","","","","Y1","Y1","Y1","Y1","Y1","Y1","Y1"]
["","Frequency","","","Hz","50","50","50","50","50","50","50"]
["","Voltage","","","V","380-415","380-415","380-415","380-415","380-415","380-415","380-415"]
["Notes","","","","","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent refrigerant piping: 5m; level difference: 0m; indoor unit fan speed: high.","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent refrigerant piping: 5m; level difference: 0m; indoor unit fan speed: high.","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent refrigerant piping: 5m; level difference: 0m; indoor unit fan speed: high.","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent refrigerant piping: 5m; level difference: 0m; indoor unit fan speed: high.","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent refrigerant piping: 5m; level difference: 0m; indoor unit fan speed: high.","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent refrigerant piping: 5m; level difference: 0m; indoor unit fan speed: high.","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent refrigerant piping: 5m; level difference: 0m; indoor unit fan speed: high."]
["","","","","","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m; level difference: 0m; indoor unit fan speed: high.","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m; level difference: 0m; indoor unit fan speed: high.","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m; level difference: 0m; indoor unit fan speed: high.","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m; level difference: 0m; indoor unit fan speed: high.","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m; level difference: 0m; indoor unit fan speed: high.","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m; level difference: 0m; indoor unit fan speed: high.","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m; level difference: 0m; indoor unit fan speed: high."]
["","","","","","(3) - Actual number of connectable indoor units depends on the indoor unit type and the connection ratio restriction for the system (50% ≤ CR ≤ 120%)","(3) - Actual number of connectable indoor units depends on the indoor unit type and the connection ratio restriction for the system (50% ≤ CR ≤ 120%)","(3) - Actual number of connectable indoor units depends on the indoor unit type and the connection ratio restriction for the system (50% ≤ CR ≤ 120%)","(3) - Actual number of connectable indoor units depends on the indoor unit type and the connection ratio restriction for the system (50% ≤ CR ≤ 120%)","(3) - Actual number of connectable indoor units depends on the indoor unit type and the connection ratio restriction for the system (50% ≤ CR ≤ 120%)","(3) - Actual number of connectable indoor units depends on the indoor unit type and the connection ratio restriction for the system (50% ≤ CR ≤ 120%)","(3) - Actual number of connectable indoor units depends on the indoor unit type and the connection ratio restriction for the system (50% ≤ CR ≤ 120%)"]
["","","","","","(4) - The maximum capacities for RXYCQ8A7Y1B and RXYCQ10A7Y1B can be up to 240 and 300 respectively if no FXFQ20/25 indoor units are present in the setup.","(4) - The maximum capacities for RXYCQ8A7Y1B and RXYCQ10A7Y1B can be up to 240 and 300 respectively if no FXFQ20/25 indoor units are present in the setup.","(4) - The maximum capacities for RXYCQ8A7Y1B and RXYCQ10A7Y1B can be up to 240 and 300 respectively if no FXFQ20/25 indoor units are present in the setup.","(4) - The maximum capacities for RXYCQ8A7Y1B and RXYCQ10A7Y1B can be up to 240 and 300 respectively if no FXFQ20/25 indoor units are present in the setup.","(4) - The maximum capacities for RXYCQ8A7Y1B and RXYCQ10A7Y1B can be up to 240 and 300 respectively if no FXFQ20/25 indoor units are present in the setup.","(4) - The maximum capacities for RXYCQ8A7Y1B and RXYCQ10A7Y1B can be up to 240 and 300 respectively if no FXFQ20/25 indoor units are present in the setup.","(4) - The maximum capacities for RXYCQ8A7Y1B and RXYCQ10A7Y1B can be up to 240 and 300 respectively if no FXFQ20/25 indoor units are present in the setup."]
["","","","","","(5) - Sound power level is an absolute value that a sound source generates.","(5) - Sound power level is an absolute value that a sound source generates.","(5) - Sound power level is an absolute value that a sound source generates.","(5) - Sound power level is an absolute value that a sound source generates.","(5) - Sound power level is an absolute value that a sound source generates.","(5) - Sound power level is an absolute value that a sound source generates.","(5) - Sound power level is an absolute value that a sound source generates."]
["","","","","","(6) - Sound pressure level is a relative value, depending on the distance and acoustic environment. For more details, please refer to the sound level drawings.","(6) - Sound pressure level is a relative value, depending on the distance and acoustic environment. For more details, please refer to the sound level drawings.","(6) - Sound pressure level is a relative value, depending on the distance and acoustic environment. For more details, please refer to the sound level drawings.","(6) - Sound pressure level is a relative value, depending on the distance and acoustic environment. For more details, please refer to the sound level drawings.","(6) - Sound pressure level is a relative value, depending on the distance and acoustic environment. For more details, please refer to the sound level drawings.","(6) - Sound pressure level is a relative value, depending on the distance and acoustic environment. For more details, please refer to the sound level drawings.","(6) - Sound pressure level is a relative value, depending on the distance and acoustic environment. For more details, please refer to the sound level drawings."]
["","","","","","(7) - Sound values are measured in a semi-anechoic room.","(7) - Sound values are measured in a semi-anechoic room.","(7) - Sound values are measured in a semi-anechoic room.","(7) - Sound values are measured in a semi-anechoic room.","(7) - Sound values are measured in a semi-anechoic room.","(7) - Sound values are measured in a semi-anechoic room.","(7) - Sound values are measured in a semi-anechoic room."]
["","","","","","(8) - Refer to refrigerant pipe selection or installation manual","(8) - Refer to refrigerant pipe selection or installation manual","(8) - Refer to refrigerant pipe selection or installation manual","(8) - Refer to refrigerant pipe selection or installation manual","(8) - Refer to refrigerant pipe selection or installation manual","(8) - Refer to refrigerant pipe selection or installation manual","(8) - Refer to refrigerant pipe selection or installation manual"]
["","","","","","(9) - For detailed contents of standard accessories see Installation manual.","(9) - For detailed contents of standard accessories see Installation manual.","(9) - For detailed contents of standard accessories see Installation manual.","(9) - For detailed contents of standard accessories see Installation manual.","(9) - For detailed contents of standard accessories see Installation manual.","(9) - For detailed contents of standard accessories see Installation manual.","(9) - For detailed contents of standard accessories see Installation manual."]
["","","","","","(10) - RLA is based on nominal conditions","(10) - RLA is based on nominal conditions","(10) - RLA is based on nominal conditions","(10) - RLA is based on nominal conditions","(10) - RLA is based on nominal conditions","(10) - RLA is based on nominal conditions","(10) - RLA is based on nominal conditions"]
["","","","","","(11) - MSC means the maximum current during start up of the compressor","(11) - MSC means the maximum current during start up of the compressor","(11) - MSC means the maximum current during start up of the compressor","(11) - MSC means the maximum current during start up of the compressor","(11) - MSC means the maximum current during start up of the compressor","(11) - MSC means the maximum current during start up of the compressor","(11) - MSC means the maximum current during start up of the compressor"]
["","","","","","(12) - MCA must be used to select the correct field wiring size. The MCA can be regarded as the maximum running current.","(12) - MCA must be used to select the correct field wiring size. The MCA can be regarded as the maximum running current.","(12) - MCA must be used to select the correct field wiring size. The MCA can be regarded as the maximum running current.","(12) - MCA must be used to select the correct field wiring size. The MCA can be regarded as the maximum running current.","(12) - MCA must be used to select the correct field wiring size. The MCA can be regarded as the maximum running current.","(12) - MCA must be used to select the correct field wiring size. The MCA can be regarded as the maximum running current.","(12) - MCA must be used to select the correct field wiring size. The MCA can be regarded as the maximum running current."]
["","","","","","(13) - MFA is used to select the circuit breaker and the ground fault circuit interrupter (earth leakage circuit breaker).","(13) - MFA is used to select the circuit breaker and the ground fault circuit interrupter (earth leakage circuit breaker).","(13) - MFA is used to select the circuit breaker and the ground fault circuit interrupter (earth leakage circuit breaker).","(13) - MFA is used to select the circuit breaker and the ground fault circuit interrupter (earth leakage circuit breaker).","(13) - MFA is used to select the circuit breaker and the ground fault circuit interrupter (earth leakage circuit breaker).","(13) - MFA is used to select the circuit breaker and the ground fault circuit interrupter (earth leakage circuit breaker).","(13) - MFA is used to select the circuit breaker and the ground fault circuit interrupter (earth leakage circuit breaker)."]
["","","","","","(14) - TOCA means the total value of each OC set.","(14) - TOCA means the total value of each OC set.","(14) - TOCA means the total value of each OC set.","(14) - TOCA means the total value of each OC set.","(14) - TOCA means the total value of each OC set.","(14) - TOCA means the total value of each OC set.","(14) - TOCA means the total value of each OC set."]
["","","","","","(15) - FLA means the nominal running current of the fan","(15) - FLA means the nominal running current of the fan","(15) - FLA means the nominal running current of the fan","(15) - FLA means the nominal running current of the fan","(15) - FLA means the nominal running current of the fan","(15) - FLA means the nominal running current of the fan","(15) - FLA means the nominal running current of the fan"]
["","","","","","(16) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(16) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(16) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(16) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(16) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(16) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(16) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits."]
["","","","","","(17) - Maximum allowable voltage range variation between phases is 2%.","(17) - Maximum allowable voltage range variation between phases is 2%.","(17) - Maximum allowable voltage range variation between phases is 2%.","(17) - Maximum allowable voltage range variation between phases is 2%.","(17) - Maximum allowable voltage range variation between phases is 2%.","(17) - Maximum allowable voltage range variation between phases is 2%.","(17) - Maximum allowable voltage range variation between phases is 2%."]
["","","","","","(18) - Contains fluorinated greenhouse gases","(18) - Contains fluorinated greenhouse gases","(18) - Contains fluorinated greenhouse gases","(18) - Contains fluorinated greenhouse gases","(18) - Contains fluorinated greenhouse gases","(18) - Contains fluorinated greenhouse gases","(18) - Contains fluorinated greenhouse gases"]
["","","","","","(19) - In accordance with EN/IEC 61000-3-11, respectively EN/IEC 61000-3-12, it may be necessary to consult the distribution network operator to ensure that the equipment is connected only to a supply with Zsys ≤ Zmax, respectively Ssc ≥ minimum Ssc value.","(19) - In accordance with EN/IEC 61000-3-11, respectively EN/IEC 61000-3-12, it may be necessary to consult the distribution network operator to ensure that the equipment is connected only to a supply with Zsys ≤ Zmax, respectively Ssc ≥ minimum Ssc value.","(19) - In accordance with EN/IEC 61000-3-11, respectively EN/IEC 61000-3-12, it may be necessary to consult the distribution network operator to ensure that the equipment is connected only to a supply with Zsys ≤ Zmax, respectively Ssc ≥ minimum Ssc value.","(19) - In accordance with EN/IEC 61000-3-11, respectively EN/IEC 61000-3-12, it may be necessary to consult the distribution network operator to ensure that the equipment is connected only to a supply with Zsys ≤ Zmax, respectively Ssc ≥ minimum Ssc value.","(19) - In accordance with EN/IEC 61000-3-11, respectively EN/IEC 61000-3-12, it may be necessary to consult the distribution network operator to ensure that the equipment is connected only to a supply with Zsys ≤ Zmax, respectively Ssc ≥ minimum Ssc value.","(19) - In accordance with EN/IEC 61000-3-11, respectively EN/IEC 61000-3-12, it may be necessary to consult the distribution network operator to ensure that the equipment is connected only to a supply with Zsys ≤ Zmax, respectively Ssc ≥ minimum Ssc value.","(19) - In accordance with EN/IEC 61000-3-11, respectively EN/IEC 61000-3-12, it may be necessary to consult the distribution network operator to ensure that the equipment is connected only to a supply with Zsys ≤ Zmax, respectively Ssc ≥ minimum Ssc value."]
["","","","","","(20) - EN/IEC 61000-3-11: European/international technical standard setting the limits for voltage changes, voltage fluctuations and flicker in public low-voltage supply systems for equipment with rated ≤ 75A","(20) - EN/IEC 61000-3-11: European/international technical standard setting the limits for voltage changes, voltage fluctuations and flicker in public low-voltage supply systems for equipment with rated ≤ 75A","(20) - EN/IEC 61000-3-11: European/international technical standard setting the limits for voltage changes, voltage fluctuations and flicker in public low-voltage supply systems for equipment with rated ≤ 75A","(20) - EN/IEC 61000-3-11: European/international technical standard setting the limits for voltage changes, voltage fluctuations and flicker in public low-voltage supply systems for equipment with rated ≤ 75A","(20) - EN/IEC 61000-3-11: European/international technical standard setting the limits for voltage changes, voltage fluctuations and flicker in public low-voltage supply systems for equipment with rated ≤ 75A","(20) - EN/IEC 61000-3-11: European/international technical standard setting the limits for voltage changes, voltage fluctuations and flicker in public low-voltage supply systems for equipment with rated ≤ 75A","(20) - EN/IEC 61000-3-11: European/international technical standard setting the limits for voltage changes, voltage fluctuations and flicker in public low-voltage supply systems for equipment with rated ≤ 75A"]
["","","","","","(21) - EN/IEC 61000-3-12: European/international technical standard setting the limits for harmonic currents produced by equipment connected to public low-voltage system with input current > 16A and ≤ 75A per phase","(21) - EN/IEC 61000-3-12: European/international technical standard setting the limits for harmonic currents produced by equipment connected to public low-voltage system with input current > 16A and ≤ 75A per phase","(21) - EN/IEC 61000-3-12: European/international technical standard setting the limits for harmonic currents produced by equipment connected to public low-voltage system with input current > 16A and ≤ 75A per phase","(21) - EN/IEC 61000-3-12: European/international technical standard setting the limits for harmonic currents produced by equipment connected to public low-voltage system with input current > 16A and ≤ 75A per phase","(21) - EN/IEC 61000-3-12: European/international technical standard setting the limits for harmonic currents produced by equipment connected to public low-voltage system with input current > 16A and ≤ 75A per phase","(21) - EN/IEC 61000-3-12: European/international technical standard setting the limits for harmonic currents produced by equipment connected to public low-voltage system with input current > 16A and ≤ 75A per phase","(21) - EN/IEC 61000-3-12: European/international technical standard setting the limits for harmonic currents produced by equipment connected to public low-voltage system with input current > 16A and ≤ 75A per phase"]
["","","","","","(22) - Short-circuit power","(22) - Short-circuit power","(22) - Short-circuit power","(22) - Short-circuit power","(22) - Short-circuit power","(22) - Short-circuit power","(22) - Short-circuit power"]
["","","","","","(23) - system impedance","(23) - system impedance","(23) - system impedance","(23) - system impedance","(23) - system impedance","(23) - system impedance","(23) - system impedance"]
["","","","","","(24) - For RXYCQ8 and RXYCQ10 MSC ≤ MCA","(24) - For RXYCQ8 and RXYCQ10 MSC ≤ MCA","(24) - For RXYCQ8 and RXYCQ10 MSC ≤ MCA","(24) - For RXYCQ8 and RXYCQ10 MSC ≤ MCA","(24) - For RXYCQ8 and RXYCQ10 MSC ≤ MCA","(24) - For RXYCQ8 and RXYCQ10 MSC ≤ MCA","(24) - For RXYCQ8 and RXYCQ10 MSC ≤ MCA"]