{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":12,"n_cols":14,"rows_kept":12,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATB-S"]
[]
[]
[]
[]
["","","","","SB.ATB05LBS","SB.ATB05RBS","SB.ATB06LBS","SB.ATB06RBS","SB.ATB07LBS","SB.ATB07RBS","ATB03LBSNADBT00","ATB03RBSNADBT00","ATB04LBSNADBT00","ATB04RBSNADBT00"]
["Nominal air flow","Return air flow","","m³/s","0.639","0.639","0.750","0.750","1.083","1.083","0.222","0.222","0.458","0.458"]
["","Supply air flow","","m³/s","0.639","0.639","0.75","0.75","1.083","1.083","0.222","0.222","0.458","0.458"]
["Dimensions","Unit","Height","mm","1750","1750","1700","1700","1900","1900","1450","1450","1450","1450"]
["","","Width","mm","790","790","790","790","890","890","550","550","790","790"]
["","","Length with damper","mm","2170","2170","2620","2620","2950","2950","1580","1580","1650","1650"]
["Supply filter","Primary filter","Class","","F7","F7","F7","F7","F7","F7","F7","F7","F7","F7"]